# Function _mm_mask_compressstoreu_ps

1.89.0 · Source

    pub unsafe fn _mm_mask_compressstoreu_ps(
        base_addr: *mut f32,
        k: __mmask8,
        a: __m128,
    )

Available on (x86 or x86-64) and target feature `avx512f` and target feature `avx512vl` and x86 only.
Expand description

Contiguously store the active single-precision (32-bit) floating-point elements in a (those with their respective bit set in writemask k) to unaligned memory at base_addr.

Intel’s documentation