## Keyboard shortcuts

Press `←` or `→` to navigate between chapters

Press `S` or `/` to search in the book

Press `?` to show this help

Press `Esc` to hide this help

# A First Attempt

## The Registers

Let's look at the 'SysTick' peripheral - a simple timer which comes with every Cortex-M processor core. Typically you'll be looking these up in the chip manufacturer's data sheet or Technical Reference Manual, but this example is common to all ARM Cortex-M cores, let's look in the ARM reference manual. We see there are four registers:

Offset | Name | Description | Width
--- | --- | --- | ---
0x00 | SYST_CSR | Control and Status Register | 32 bits
0x04 | SYST_RVR | Reload Value Register | 32 bits
0x08 | SYST_CVR | Current Value Register | 32 bits
0x0C | SYST_CALIB | Calibration Value Register | 32 bits

## The C Approach

In Rust, we can represent a collection of registers in exactly the same way as we do in C - with a `struct`.

    #[repr(C)]
    struct SysTick {
        pub csr: u32,
        pub rvr: u32,
        pub cvr: u32,
        pub calib: u32,
    }

The qualifier `#[repr(C)]` tells the Rust compiler to lay this structure out like a C compiler would. That's very important, as Rust allows structure fields to be re-ordered, while C does not. You can imagine the debugging we'd have to do if these fields were silently re-arranged by the compiler! With this qualifier in place, we have our four 32-bit fields which correspond to the table above. But of course, this `struct` is of no use by itself - we need a variable.

    let systick = 0xE000_E010 as *mut SysTick;
    let time = unsafe { (*systick).cvr };

## Volatile Accesses

Now, there are a couple of problems with the approach above.

1. We have to use unsafe every time we want to access our Peripheral.
2. We've got no way of specifying which registers are read-only or read-write.
3. Any piece of code anywhere in your program could access the hardware through this structure.
4. Most importantly, it doesn't actually work...

Now, the problem is that compilers are clever. If you make two writes to the same piece of RAM, one after the other, the compiler can notice this and just skip the first write entirely. In C, we can mark variables as `volatile` to ensure that every read or write occurs as intended. In Rust, we instead mark the accesses as volatile, not the variable.

    let systick = unsafe { &mut *(0xE000_E010 as *mut SysTick) };
    let time = unsafe { core::ptr::read_volatile(&mut systick.cvr) };

So, we've fixed one of our four problems, but now we have even more `unsafe` code! Fortunately, there's a third party crate which can help - `volatile_register`.

    use volatile_register::{RW, RO};

    #[repr(C)]
    struct SysTick {
        pub csr: RW<u32>,
        pub rvr: RW<u32>,
        pub cvr: RW<u32>,
        pub calib: RO<u32>,
    }

    fn get_systick() -> &'static mut SysTick {
        unsafe { &mut *(0xE000_E010 as *mut SysTick) }
    }

    fn get_time() -> u32 {
        let systick = get_systick();
        systick.cvr.read()
    }

Now, the volatile accesses are performed automatically through the `read` and `write` methods. It's still `unsafe` to perform writes, but to be fair, hardware is a bunch of mutable state and there's no way for the compiler to know whether these writes are actually safe, so this is a good default position.

## The Rusty Wrapper

We need to wrap this `struct` up into a higher-layer API that is safe for our users to call. As the driver author, we manually verify the unsafe code is correct, and then present a safe API for our users so they don't have to worry about it (provided they trust us to get it right!).

One example might be:

    use volatile_register::{RW, RO};

    pub struct SystemTimer {
        p: &'static mut RegisterBlock
    }

    #[repr(C)]
    struct RegisterBlock {
        pub csr: RW<u32>,
        pub rvr: RW<u32>,
        pub cvr: RW<u32>,
        pub calib: RO<u32>,
    }

    impl SystemTimer {
        pub fn new() -> SystemTimer {
            SystemTimer {
                p: unsafe { &mut *(0xE000_E010 as *mut RegisterBlock) }
            }
        }

        pub fn get_time(&self) -> u32 {
            self.p.cvr.read()
        }

        pub fn set_reload(&mut self, reload_value: u32) {
            unsafe { self.p.rvr.write(reload_value) }
        }
    }

    pub fn example_usage() -> String {
        let mut st = SystemTimer::new();
        st.set_reload(0x00FF_FFFF);
        format!("Time is now 0x{:08x}", st.get_time())
    }

Now, the problem with this approach is that the following code is perfectly acceptable to the compiler:

    fn thread1() {
        let mut st = SystemTimer::new();
        st.set_reload(2000);
    }

    fn thread2() {
        let mut st = SystemTimer::new();
        st.set_reload(1000);
    }

Our `&mut self` argument to the `set_reload` function checks that there are no other references to that particular `SystemTimer` struct, but they don't stop the user creating a second `SystemTimer` which points to the exact same peripheral! Code written in this fashion will work if the author is diligent enough to spot all of these 'duplicate' driver instances, but once the code is spread out over multiple modules, drivers, developers, and days, it gets easier and easier to make these kinds of mistakes.