# Function _mm_maskz_min_ph

Source

    pub fn _mm_maskz_min_ph(k: __mmask8, a: __m128h, b: __m128h) -> __m128h

🔬This is a nightly-only experimental API. (`stdarch_x86_avx512_f16` #127213)
Available on (x86 or x86-64) and target feature `avx512fp16` and target feature `avx512vl` and x86 only.
Expand description

Compare packed half-precision (16-bit) floating-point elements in a and b, and store packed minimum values in dst using zeromask k (elements are zeroed out when the corresponding mask bit is not set). Does not follow the IEEE Standard for Floating-Point Arithmetic (IEEE 754) minimum value when inputs are NaN or signed-zero values.

Intel’s documentation