# Function _mm512_mask_cvtepi32_epi8

1.89.0 · Source

    pub fn _mm512_mask_cvtepi32_epi8(
        src: __m128i,
        k: __mmask16,
        a: __m512i,
    ) -> __m128i

Available on (x86 or x86-64) and target feature `avx512f` and x86 only.
Expand description

Convert packed 32-bit integers in a to packed 8-bit integers with truncation, and store the results in dst using writemask k (elements are copied from src when the corresponding mask bit is not set).

Intel’s documentation