# Function _mm512_multishift_epi64_epi8

1.89.0 · Source

    pub fn _mm512_multishift_epi64_epi8(a: __m512i, b: __m512i) -> __m512i

Available on (x86 or x86-64) and target feature `avx512vbmi` and x86-64 only.
Expand description

For each 64-bit element in b, select 8 unaligned bytes using a byte-granular shift control within the corresponding 64-bit element of a, and store the 8 assembled bytes to the corresponding 64-bit element of dst.

Intel’s documentation