# Function _mm512_maskz_permutexvar_epi8

1.89.0 · Source

    pub fn _mm512_maskz_permutexvar_epi8(
        k: __mmask64,
        idx: __m512i,
        a: __m512i,
    ) -> __m512i

Available on (x86 or x86-64) and target feature `avx512vbmi` and x86-64 only.
Expand description

Shuffle 8-bit integers in a across lanes using the corresponding index in idx, and store the results in dst using zeromask k (elements are zeroed out when the corresponding mask bit is not set).

Intel’s documentation