# Function _mm512_mask_cvtusepi16_epi8

1.89.0 · Source

    pub fn _mm512_mask_cvtusepi16_epi8(
        src: __m256i,
        k: __mmask32,
        a: __m512i,
    ) -> __m256i

Available on (x86 or x86-64) and target feature `avx512bw` and x86-64 only.
Expand description

Convert packed unsigned 16-bit integers in a to packed unsigned 8-bit integers with unsigned saturation, and store the results in dst using writemask k (elements are copied from src when the corresponding mask bit is not set).

Intel’s documentation