# Function _mm_maskz_compress_epi8

1.89.0 · Source

    pub fn _mm_maskz_compress_epi8(k: __mmask16, a: __m128i) -> __m128i

Available on (x86 or x86-64) and target feature `avx512vbmi2` and target feature `avx512vl` and x86 only.
Expand description

Contiguously store the active 8-bit integers in a (those with their respective bit set in zeromask k) to dst, and set the remaining elements to zero.

Intel’s documentation