# Function _mm512_mask_compressstoreu_epi8

1.89.0 · Source

    pub unsafe fn _mm512_mask_compressstoreu_epi8(
        base_addr: *mut i8,
        k: __mmask64,
        a: __m512i,
    )

Available on (x86 or x86-64) and target feature `avx512vbmi2` and x86 only.
Expand description

Contiguously store the active 8-bit integers in a (those with their respective bit set in writemask k) to unaligned memory at base_addr.

Intel’s documentation