# Function _mm512_mask_expandloadu_epi8

1.89.0 · Source

    pub unsafe fn _mm512_mask_expandloadu_epi8(
        src: __m512i,
        k: __mmask64,
        mem_addr: *const i8,
    ) -> __m512i

Available on (x86 or x86-64) and target feature `avx512vbmi2` and x86 only.
Expand description

Load contiguous active 8-bit integers from unaligned memory at mem_addr (those with their respective bit set in mask k), and store the results in dst using writemask k (elements are copied from src when the corresponding mask bit is not set).

Intel’s documentation