# Function _kortest_mask16_u8

1.89.0 · Source

    pub unsafe fn _kortest_mask16_u8(
        a: __mmask16,
        b: __mmask16,
        all_ones: *mut u8,
    ) -> u8

Available on (x86 or x86-64) and target feature `avx512f` and x86-64 only.
Expand description

Compute the bitwise OR of 16-bit masks a and b. If the result is all zeros, store 1 in dst, otherwise store 0 in dst. If the result is all ones, store 1 in all_ones, otherwise store 0 in all_ones.

Intel’s Documentation