# Function _mm512_insertf32x8

1.89.0 · Source

    pub fn _mm512_insertf32x8(a: __m512, b: __m256, const IMM8: i32) -> __m512

Available on (x86 or x86-64) and target feature `avx512dq` and x86 only.
Expand description

Copy a to dst, then insert 256 bits (composed of 8 packed single-precision (32-bit) floating-point elements) from b into dst at the location specified by IMM8.

Intel’s Documentation