# Function _mm512_maskz_broadcast_f32x8

1.89.0 · Source

    pub fn _mm512_maskz_broadcast_f32x8(k: __mmask16, a: __m256) -> __m512

Available on (x86 or x86-64) and target feature `avx512dq` and x86 only.
Expand description

Broadcasts the 8 packed single-precision (32-bit) floating-point elements from a to all elements of dst using zeromask k (elements are zeroed out if the corresponding bit is not set).

Intel’s Documentation