# Function _mm512_maskz_adds_epu8

1.89.0 · Source

    pub fn _mm512_maskz_adds_epu8(k: __mmask64, a: __m512i, b: __m512i) -> __m512i

Available on (x86 or x86-64) and target feature `avx512bw` and x86 only.
Expand description

Add packed unsigned 8-bit integers in a and b using saturation, and store the results in dst using zeromask k (elements are zeroed out when the corresponding mask bit is not set).

Intel’s documentation