# Function _mm_mask_adds_epu8

1.89.0 · Source

    pub fn _mm_mask_adds_epu8(
        src: __m128i,
        k: __mmask16,
        a: __m128i,
        b: __m128i,
    ) -> __m128i

Available on (x86 or x86-64) and target feature `avx512bw` and target feature `avx512vl` and x86 only.
Expand description

Add packed unsigned 8-bit integers in a and b using saturation, and store the results in dst using writemask k (elements are copied from src when the corresponding mask bit is not set).

Intel’s documentation