# Function _mm_testnzc_pd

1.27.0 · Source

    pub fn _mm_testnzc_pd(a: __m128d, b: __m128d) -> i32

Available on (x86 or x86-64) and target feature `avx` and x86 only.
Expand description

Computes the bitwise AND of 128 bits (representing double-precision (64-bit) floating-point elements) in `a` and `b`, producing an intermediate 128-bit value, and set `ZF` to 1 if the sign bit of each 64-bit element in the intermediate value is zero, otherwise set `ZF` to 0. Compute the bitwise NOT of `a` and then AND with `b`, producing an intermediate value, and set `CF` to 1 if the sign bit of each 64-bit element in the intermediate value is zero, otherwise set `CF` to 0. Return 1 if both the `ZF` and `CF` values are zero, otherwise return 0.

Intel’s documentation