# Function _mm512_mask_sub_pd

1.89.0 · Source

    pub fn _mm512_mask_sub_pd(
        src: __m512d,
        k: __mmask8,
        a: __m512d,
        b: __m512d,
    ) -> __m512d

Available on (x86 or x86-64) and target feature `avx512f` and x86-64 only.
Expand description

Subtract packed double-precision (64-bit) floating-point elements in b from packed double-precision (64-bit) floating-point elements in a, and store the results in dst using writemask k (elements are copied from src when the corresponding mask bit is not set).

Intel’s documentation