# Function _mm512_load_pd

1.89.0 · Source

    pub unsafe fn _mm512_load_pd(mem_addr: *const f64) -> __m512d

Available on (x86 or x86-64) and target feature `avx512f` and x86 only.
Expand description

Load 512-bits (composed of 8 packed double-precision (64-bit) floating-point elements) from memory into dst. mem_addr must be aligned on a 64-byte boundary or a general-protection exception may be generated.

Intel’s documentation