7,6 +187,8 @@ stable kernels.
 +----------------+-----------------+-----------------+-----------------------------+
 | ARM            | Neoverse-V3     | #3312417        | ARM64_ERRATUM_3194386       |
 +----------------+-----------------+-----------------+-----------------------------+
+| ARM            | Neoverse-V3AE   | #3312417        | ARM64_ERRATUM_3194386       |
++----------------+-----------------+-----------------+-----------------------------+
 | ARM            | MMU-500         | #841119,826419  | N/A                         |
 +----------------+-----------------+-----------------+-----------------------------+
 | ARM            | MMU-600         | #1076982,1209401| N/A                         |
diff --git a/Documentation/networking/seg6-sysctl.rst b/Documentation/networking/seg6-sysctl.rst
index 07c20e470baf..1b6af4779be1 100644
--- a/Documentation/networking/seg6-sysctl.rst
+++ b/Documentation/networking/seg6-sysctl.rst
@@ -25,6 +25,9 @@ seg6_require_hmac - INTEGER
 
 	Default is 0.
 
+/proc/sys/net/ipv6/seg6_* variables:
+====================================
+
 seg6_flowlabel - INTEGER
 	Controls the behaviour of computing the flowlabel of outer
 	IPv6 header in case of SR T.encaps
diff --git a/Makefile b/Makefile
index ab277ff87643..ad3952fb542d 100644
--- a/Makefile
+++ b/Makefile
@@ -1,7 +1,7 @@
 # SPDX-License-Identifier: GPL-2.0
 VERSION = 6
 PATCHLEVEL = 6
-SUBLEVEL = 113
+SUBLEVEL = 114
 EXTRAVERSION =
 NAME = Pinguïn Aangedreven
 
diff --git a/arch/arm64/Kconfig b/arch/arm64/Kconfig
index 4ecba0690938..1be9f1f6b320 100644
--- a/arch/arm64/Kconfig
+++ b/arch/arm64/Kconfig
@@ -1094,6 +1094,7 @@ config ARM64_ERRATUM_3194386
 	  * ARM Neoverse-V1 erratum 3324341
 	  * ARM Neoverse V2 erratum 3324336
 	  * ARM Neoverse-V3 erratum 3312417
+	  * ARM Neoverse-V3AE erratum 3312417
 
 	  On affected cores "MSR SSBS, #0" instructions may not affect
 	  subsequent speculative instructions, which may permit unexepected
diff --git a/arch/arm64/include/asm/cputype.h b/arch/arm64/include/asm/cputype.h
index d92a0203e5a9..c279a0a9b366 100644
--- a/arch/arm64/include/asm/cputype.h
+++ b/arch/arm64/include/asm/cputype.h
@@ -93,6 +93,7 @@
 #define ARM_CPU_PART_NEOVERSE_V2	0xD4F
 #define ARM_CPU_PART_CORTEX_A720	0xD81
 #define ARM_CPU_PART_CORTEX_X4		0xD82
+#define ARM_CPU_PART_NEOVERSE_V3AE	0xD83
 #define ARM_CPU_PART_NEOVERSE_V3	0xD84
 #define ARM_CPU_PART_CORTEX_X925	0xD85
 #define ARM_CPU_PART_CORTEX_A725	0xD87
@@ -180,6 +181,7 @@
 #define MIDR_NEOVERSE_V2 MIDR_CPU_MODEL(ARM_CPU_IMP_ARM, ARM_CPU_PART_NEOVERSE_V2)
 #define MIDR_CORTEX_A720 MIDR_CPU_MODEL(ARM_CPU_IMP_ARM, ARM_CPU_PART_CORTEX_A720)
 #define MIDR_CORTEX_X4 MIDR_CPU_MODEL(ARM_CPU_IMP_ARM, ARM_CPU_PART_CORTEX_X4)
+#define MIDR_NEOVERSE_V3AE	MIDR_CPU_MODEL(ARM_CPU_IMP_ARM, ARM_CPU_PART_NEOVERSE_V3AE)
 #define MIDR_NEOVERSE_V3 MIDR_CPU_MODEL(ARM_CPU_IMP_ARM, ARM_CPU_PART_NEOVERSE_V3)
 #define MIDR_CORTEX_X925 MIDR_CPU_MODEL(ARM_CPU_IMP_ARM, ARM_CPU_PART_CORTEX_X925)
 #define MIDR_CORTEX_A725 MIDR_CPU_MODEL(ARM_CPU_IMP_ARM, ARM_CPU_PART_CORTEX_A725)
diff --git a/arch/arm64/kernel/cpu_errata.c b/arch/arm64/kernel/cpu_errata.c
index 463b48d0f925..23dcd0c4aad3 100644
--- a/arch/arm64/kernel/cpu_errata.c
+++ b/arch/arm64/kernel/cpu_errata.c
@@ -471,6 +471,7 @@ static const struct midr_range erratum_spec_ssbs_list[] = {
 	MIDR_ALL_VERSIONS(MIDR_NEOVERSE_V1),
 	MIDR_ALL_VERSIONS(MIDR_NEOVERSE_V2),
 	MIDR_ALL_VERSIONS(MIDR_NEOVERSE_V3),
+	MIDR_ALL_VERSIONS(MIDR_NEOVERSE_V3AE),
 	{}
 };
 #endif
diff --git a/arch/riscv/kernel/probes/kprobes.c b/arch/riscv/kernel/probes/kprobes.c
index 297427ffc4e0..8a6ea7d27018 100644
--- a/arch/riscv/kernel/probes/kprobes.c
+++ b/arch/riscv/kernel/probes/kprobes.c
@@ -48,10 +48,15 @@ static void __kprobes arch_simulate_insn(struct kprobe *p, struct pt_regs *regs)
 	post_kprobe_handler(p, kcb, regs);
 }
 
-static bool __kprobes arch_check_kprobe(struct kprobe *p)
+static bool __kprobes arch_check_kprobe(unsigned long addr)
 {
-	unsigned long tmp  = (unsigned long)p->addr - p->offset;
-	unsigned long addr = (unsigned long)p->addr;
+	unsigned long tmp, offset;
+
+	/* start iterating at the closest preceding symbol */
+	if (!kallsyms_lookup_size_offset(addr, NULL, &offset))
+		return false;
+
+	tmp = addr - offset;
 
 	while (tmp <= addr) {
 		if (tmp == addr)
@@ -70,7 +75,7 @@ int __kprobes arch_prepare_kprobe(struct kprobe *p)
 	if ((unsigned long)insn & 0x1)
 		return -EILSEQ;
 
-	if (!arch_check_kprobe(p))
+	if (!arch_check_kprobe((unsigned long)p->addr))
 		return -EILSEQ;
 
 	/* copy instruction */
diff --git a/block/bdev.c b/block/bdev.c
index 5a54977518ee..a8357b72a27b 100644
--- a/block/bdev.c
+++ b/block/bdev.c
@@ -147,9 +147,26 @@ int set_blocksize(struct block_device *bdev, int size)
 
 	/* Don't change the size if it is same as current */
 	if (bdev->bd_inode->i_blkbits != blksize_bits(size)) {
+		/*
+		 * Flush and truncate the pagecache before we reconfigure the
+		 * mapping geometry because folio sizes are variable now.  If a
+		 * reader has already allocated a folio whose size is smaller
+		 * than the new min_order but invokes readahead after the new
+		 * min_order becomes visible, readahead will think there are
+		 * "zero" blocks per folio and crash.  Take the inode and
+		 * invalidation locks to avoid racing with
+		 * read/write/fallocate.
+		 */
+		inode_lock(bdev->bd_inode);
+		filemap_invalidate_lock(bdev->bd_inode->i_mapping);
+
 		sync_blockdev(bdev);
+		kill_bdev(bdev);
+
 		bdev->bd_inode->i_blkbits = blksize_bits(size);
 		kill_bdev(bdev);
+		filemap_invalidate_unlock(bdev->bd_inode->i_mapping);
+		inode_unlock(bdev->bd_inode);
 	}
 	return 0;
 }
diff --git a/block/blk-zoned.c b/block/blk-zoned.c
index 619ee41a51cc..644bfa1f6753 100644
--- a/block/blk-zoned.c
+++ b/block/blk-zoned.c
@@ -401,6 +401,7 @@ int blkdev_zone_mgmt_ioctl(struct block_device *bdev, blk_mode_t mode,
 		op = REQ_OP_ZONE_RESET;
 
 		/* Invalidate the page cache, including dirty pages. */
+		inode_lock(bdev->bd_inode);
 		filemap_invalidate_lock(bdev->bd_inode->i_mapping);
 		ret = blkdev_truncate_zone_range(bdev, mode, &zrange);
 		if (ret)
@@ -423,8 +424,10 @@ int blkdev_zone_mgmt_ioctl(struct block_device *bdev, blk_mode_t mode,
 			       GFP_KERNEL);
 
 fail:
-	if (cmd == BLKRESETZONE)
+	if (cmd == BLKRESETZONE) {
 		filemap_invalidate_unlock(bdev->bd_inode->i_mapping);
+		inode_unlock(bdev->bd_inode);
+	}
 
 	return ret;
 }
diff --git a/block/fops.c b/block/fops.c
index 7c257eb3564d..088143fa9ac9 100644
--- a/block/fops.c
+++ b/block/fops.c
@@ -681,7 +681,14 @@ static ssize_t blkdev_write_iter(struct kiocb *iocb, struct iov_iter *from)
 			ret = direct_write_fallback(iocb, from, ret,
 					blkdev_buffered_write(iocb, from));
 	} else {
+		/*
+		 * Take i_rwsem and invalidate_lock to avoid racing with
+		 * set_blocksize changing i_blkbits/folio order and punching
+		 * out the pagecache.
+		 */
+		inode_lock_shared(bd_inode);
 		ret = blkdev_buffered_write(iocb, from);
+		inode_unlock_shared(bd_inode);
 	}
 
 	if (ret > 0)
@@ -693,6 +700,7 @@ static ssize_t blkdev_write_iter(struct kiocb *iocb, struct iov_iter *from)
 static ssize_t blkdev_read_iter(struct kiocb *iocb, struct iov_iter *to)
 {
 	struct block_device *bdev = I_BDEV(iocb->ki_filp->f_mapping->host);
+	struct inode *bd_inode = bdev->bd_inode;
 	loff_t size = bdev_nr_bytes(bdev);
 	loff_t pos = iocb->ki_pos;
 	size_t shorted = 0;
@@ -728,7 +736,13 @@ static ssize_t blkdev_read_iter(struct kiocb *iocb, struct iov_iter *to)
 			goto reexpand;
 	}
 
+	/*
+	 * Take i_rwsem and invalidate_lock to avoid racing with set_blocksize
+	 * changing i_blkbits/folio order and punching out the pagecache.
+	 */
+	inode_lock_shared(bd_inode);
 	ret = filemap_read(iocb, to, ret);
+	inode_unlock_shared(bd_inode);
 
 reexpand:
 	if (unlikely(shorted))
@@ -771,6 +785,7 @@ static long blkdev_fallocate(struct file *file, int mode, loff_t start,
 	if ((start | len) & (bdev_logical_block_size(bdev) - 1))
 		return -EINVAL;
 
+	inode_lock(inode);
 	filemap_invalidate_lock(inode->i_mapping);
 
 	/*
@@ -811,6 +826,7 @@ static long blkdev_fallocate(struct file *file, int mode, loff_t start,
 
  fail:
 	filemap_invalidate_unlock(inode->i_mapping);
+	inode_unlock(inode);
 	return error;
 }
 
diff --git a/block/ioctl.c b/block/ioctl.c
index 231537f79a8c..024767fa1e52 100644
--- a/block/ioctl.c
+++ b/block/ioctl.c
@@ -114,6 +114,7 @@ static int blk_ioctl_discard(struct block_device *bdev, blk_mode_t mode,
 	    end > bdev_nr_bytes(bdev))
 		return -EINVAL;
 
+	inode_lock(inode);
 	filemap_invalidate_lock(inode->i_mapping);
 	err = truncate_bdev_range(bdev, mode, start, end - 1);
 	if (err)
@@ -121,6 +122,7 @@ static int blk_ioctl_discard(struct block_device *bdev, blk_mode_t mode,
 	err = blkdev_issue_discard(bdev, start >> 9, len >> 9, GFP_KERNEL);
 fail:
 	filemap_invalidate_unlock(inode->i_mapping);
+	inode_unlock(inode);
 	return err;
 }
 
@@ -146,12 +148,14 @@ static int blk_ioctl_secure_erase(struct block_device *bdev, blk_mode_t mode,
 	    end > bdev_nr_bytes(bdev))
 		return -EINVAL;
 
+	inode_lock(bdev->bd_inode);
 	filemap_invalidate_lock(bdev->bd_inode->i_mapping);
 	err = truncate_bdev_range(bdev, mode, start, end - 1);
 	if (!err)
 		err = blkdev_issue_secure_erase(bdev, start >> 9, len >> 9,
 						GFP_KERNEL);
 	filemap_invalidate_unlock(bdev->bd_inode->i_mapping);
+	inode_unlock(bdev->bd_inode);
 	return err;
 }
 
@@ -184,6 +188,7 @@ static int blk_ioctl_zeroout(struct block_device *bdev, blk_mode_t mode,
 		return -EINVAL;
 
 	/* Invalidate the page cache, including dirty pages */
+	inode_lock(inode);
 	filemap_invalidate_lock(inode->i_mapping);
 	err = truncate_bdev_range(bdev, mode, start, end);
 	if (err)
@@ -194,6 +199,7 @@ static int blk_ioctl_zeroout(struct block_device *bdev, blk_mode_t mode,
 
 fail:
 	filemap_invalidate_unlock(inode->i_mapping);
+	inode_unlock(inode);
 	return err;
 }
 
diff --git a/drivers/accel/qaic/qaic_control.c b/drivers/accel/qaic/qaic_control.c
index f3db3fa91dd5..08b78f567853 100644
--- a/drivers/accel/qaic/qaic_control.c
+++ b/drivers/accel/qaic/qaic_control.c
@@ -407,7 +407,7 @@ static int find_and_map_user_pages(struct qaic_device *qdev,
 		return -EINVAL;
 	remaining = in_trans->size - resources->xferred_dma_size;
 	if (remaining == 0)
-		return 0;
+		return -EINVAL;
 
 	if (check_add_overflow(xfer_start_addr, remaining, &end))
 		return -EINVAL;
diff --git a/drivers/base/power/runtime.c b/drivers/base/power/runtime.c
index f53c14fb74fd..5a33cee9a394 100644
--- a/drivers/base/power/runtime.c
+++ b/drivers/base/power/runtime.c
@@ -1552,6 +1552,32 @@ void pm_runtime_enable(struct device *dev)
 }
 EXPORT_SYMBOL_GPL(pm_runtime_enable);
 
+static void pm_runtime_set_suspended_action(void *data)
+{
+	pm_runtime_set_suspended(data);
+}
+
+/**
+ * devm_pm_runtime_set_active_enabled - set_active version of devm_pm_runtime_enable.
+ *
+ * @dev: Device to handle.
+ */
+int devm_pm_runtime_set_active_enabled(struct device *dev)
+{
+	int err;
+
+	err = pm_runtime_set_active(dev);
+	if (err)
+		return err;
+
+	err = devm_add_action_or_reset(dev, pm_runtime_set_suspended_action, dev);
+	if (err)
+		return err;
+
+	return devm_pm_runtime_enable(dev);
+}
+EXPORT_SYMBOL_GPL(devm_pm_runtime_set_active_enabled);
+
 static void pm_runtime_disable_action(void *data)
 {
 	pm_runtime_dont_use_autosuspend(data);
@@ -1574,6 +1600,24 @@ int devm_pm_runtime_enable(struct device *dev)
 }
 EXPORT_SYMBOL_GPL(devm_pm_runtime_enable);
 
+static void pm_runtime_put_noidle_action(void *data)
+{
+	pm_runtime_put_noidle(data);
+}
+
+/**
+ * devm_pm_runtime_get_noresume - devres-enabled version of pm_runtime_get_noresume.
+ *
+ * @dev: Device to handle.
+ */
+int devm_pm_runtime_get_noresume(struct device *dev)
+{
+	pm_runtime_get_noresume(dev);
+
+	return devm_add_action_or_reset(dev, pm_runtime_put_noidle_action, dev);
+}
+EXPORT_SYMBOL_GPL(devm_pm_runtime_get_noresume);
+
 /**
  * pm_runtime_forbid - Block runtime PM of a device.
  * @dev: Device to handle.
diff --git a/drivers/bluetooth/btusb.c b/drivers/bluetooth/btusb.c
index 1a2d227b7b7b..4c21230aee46 100644
--- a/drivers/bluetooth/btusb.c
+++ b/drivers/bluetooth/btusb.c
@@ -511,6 +511,8 @@ static const struct usb_device_id quirks_table[] = {
 	/* Realtek 8851BU Bluetooth devices */
 	{ USB_DEVICE(0x3625, 0x010b), .driver_info = BTUSB_REALTEK |
 						     BTUSB_WIDEBAND_SPEECH },
+	{ USB_DEVICE(0x2001, 0x332a), .driver_info = BTUSB_REALTEK |
+						     BTUSB_WIDEBAND_SPEECH },
 
 	/* Realtek 8852AE Bluetooth devices */
 	{ USB_DEVICE(0x0bda, 0x2852), .driver_info = BTUSB_REALTEK |
diff --git a/drivers/cpufreq/cppc_cpufreq.c b/drivers/cpufreq/cppc_cpufreq.c
index ea32bdf7cc24..4d96eed64fe0 100644
--- a/drivers/cpufreq/cppc_cpufreq.c
+++ b/drivers/cpufreq/cppc_cpufreq.c
@@ -344,6 +344,16 @@ static int cppc_verify_policy(struct cpufreq_policy_data *policy)
 	return 0;
 }
 
+static unsigned int __cppc_cpufreq_get_transition_delay_us(unsigned int cpu)
+{
+	unsigned int transition_latency_ns = cppc_get_transition_latency(cpu);
+
+	if (transition_latency_ns == CPUFREQ_ETERNAL)
+		return CPUFREQ_DEFAULT_TRANSITION_LATENCY_NS / NSEC_PER_USEC;
+
+	return transition_latency_ns / NSEC_PER_USEC;
+}
+
 /*
  * The PCC subspace describes the rate at which platform can accept commands
  * on the shared PCC channel (including READs which do not count towards freq
@@ -366,12 +376,12 @@ static unsigned int cppc_cpufreq_get_transition_delay_us(unsigned int cpu)
 			return 10000;
 		}
 	}
-	return cppc_get_transition_latency(cpu) / NSEC_PER_USEC;
+	return __cppc_cpufreq_get_transition_delay_us(cpu);
 }
 #else
 static unsigned int cppc_cpufreq_get_transition_delay_us(unsigned int cpu)
 {
-	return cppc_get_transition_latency(cpu) / NSEC_PER_USEC;
+	return __cppc_cpufreq_get_transition_delay_us(cpu);
 }
 #endif
 
diff --git a/drivers/gpu/drm/amd/amdgpu/amdgpu_amdkfd_gpuvm.c b/drivers/gpu/drm/amd/amdgpu/amdgpu_amdkfd_gpuvm.c
index a1f35510d539..c94e1cc7e3a7 100644
--- a/drivers/gpu/drm/amd/amdgpu/amdgpu_amdkfd_gpuvm.c
+++ b/drivers/gpu/drm/amd/amdgpu/amdgpu_amdkfd_gpuvm.c
@@ -2285,10 +2285,9 @@ void amdgpu_amdkfd_gpuvm_unmap_gtt_bo_from_kernel(struct kgd_mem *mem)
 int amdgpu_amdkfd_gpuvm_get_vm_fault_info(struct amdgpu_device *adev,
 					  struct kfd_vm_fault_info *mem)
 {
-	if (atomic_read(&adev->gmc.vm_fault_info_updated) == 1) {
+	if (atomic_read_acquire(&adev->gmc.vm_fault_info_updated) == 1) {
 		*mem = *adev->gmc.vm_fault_info;
-		mb(); /* make sure read happened */
-		atomic_set(&adev->gmc.vm_fault_info_updated, 0);
+		atomic_set_release(&adev->gmc.vm_fault_info_updated, 0);
 	}
 	return 0;
 }
diff --git a/drivers/gpu/drm/amd/amdgpu/amdgpu_psp.c b/drivers/gpu/drm/amd/amdgpu/amdgpu_psp.c
index c83445c2e37f..d358a08b5e00 100644
--- a/drivers/gpu/drm/amd/amdgpu/amdgpu_psp.c
+++ b/drivers/gpu/drm/amd/amdgpu/amdgpu_psp.c
@@ -2012,7 +2012,7 @@ static int psp_securedisplay_initialize(struct psp_context *psp)
 	}
 
 	ret = psp_ta_load(psp, &psp->securedisplay_context.context);
-	if (!ret) {
+	if (!ret && !psp->securedisplay_context.context.resp_status) {
 		psp->securedisplay_context.context.initialized = true;
 		mutex_init(&psp->securedisplay_context.mutex);
 	} else
diff --git a/drivers/gpu/drm/amd/amdgpu/gmc_v7_0.c b/drivers/gpu/drm/amd/amdgpu/gmc_v7_0.c
index fd905889a4c6..e2ee10a98640 100644
--- a/drivers/gpu/drm/amd/amdgpu/gmc_v7_0.c
+++ b/drivers/gpu/drm/amd/amdgpu/gmc_v7_0.c
@@ -1061,7 +1061,7 @@ static int gmc_v7_0_sw_init(void *handle)
 					GFP_KERNEL);
 	if (!adev->gmc.vm_fault_info)
 		return -ENOMEM;
-	atomic_set(&adev->gmc.vm_fault_info_updated, 0);
+	atomic_set_release(&adev->gmc.vm_fault_info_updated, 0);
 
 	return 0;
 }
@@ -1290,7 +1290,7 @@ static int gmc_v7_0_process_interrupt(struct amdgpu_device *adev,
 	vmid = REG_GET_FIELD(status, VM_CONTEXT1_PROTECTION_FAULT_STATUS,
 			     VMID);
 	if (amdgpu_amdkfd_is_kfd_vmid(adev, vmid)
-		&& !atomic_read(&adev->gmc.vm_fault_info_updated)) {
+		&& !atomic_read_acquire(&adev->gmc.vm_fault_info_updated)) {
 		struct kfd_vm_fault_info *info = adev->gmc.vm_fault_info;
 		u32 protections = REG_GET_FIELD(status,
 					VM_CONTEXT1_PROTECTION_FAULT_STATUS,
@@ -1306,8 +1306,7 @@ static int gmc_v7_0_process_interrupt(struct amdgpu_device *adev,
 		info->prot_read = protections & 0x8 ? true : false;
 		info->prot_write = protections & 0x10 ? true : false;
 		info->prot_exec = protections & 0x20 ? true : false;
-		mb();
-		atomic_set(&adev->gmc.vm_fault_info_updated, 1);
+		atomic_set_release(&adev->gmc.vm_fault_info_updated, 1);
 	}
 
 	return 0;
diff --git a/drivers/gpu/drm/amd/amdgpu/gmc_v8_0.c b/drivers/gpu/drm/amd/amdgpu/gmc_v8_0.c
index 0bebcdbb2658..ed268c5739eb 100644
--- a/drivers/gpu/drm/amd/amdgpu/gmc_v8_0.c
+++ b/drivers/gpu/drm/amd/amdgpu/gmc_v8_0.c
@@ -1174,7 +1174,7 @@ static int gmc_v8_0_sw_init(void *handle)
 					GFP_KERNEL);
 	if (!adev->gmc.vm_fault_info)
 		return -ENOMEM;
-	atomic_set(&adev->gmc.vm_fault_info_updated, 0);
+	atomic_set_release(&adev->gmc.vm_fault_info_updated, 0);
 
 	return 0;
 }
@@ -1465,7 +1465,7 @@ static int gmc_v8_0_process_interrupt(struct amdgpu_device *adev,
 	vmid = REG_GET_FIELD(status, VM_CONTEXT1_PROTECTION_FAULT_STATUS,
 			     VMID);
 	if (amdgpu_amdkfd_is_kfd_vmid(adev, vmid)
-		&& !atomic_read(&adev->gmc.vm_fault_info_updated)) {
+		&& !atomic_read_acquire(&adev->gmc.vm_fault_info_updated)) {
 		struct kfd_vm_fault_info *info = adev->gmc.vm_fault_info;
 		u32 protections = REG_GET_FIELD(status,
 					VM_CONTEXT1_PROTECTION_FAULT_STATUS,
@@ -1481,8 +1481,7 @@ static int gmc_v8_0_process_interrupt(struct amdgpu_device *adev,
 		info->prot_read = protections & 0x8 ? true : false;
 		info->prot_write = protections & 0x10 ? true : false;
 		info->prot_exec = protections & 0x20 ? true : false;
-		mb();
-		atomic_set(&adev->gmc.vm_fault_info_updated, 1);
+		atomic_set_release(&adev->gmc.vm_fault_info_updated, 1);
 	}
 
 	return 0;
diff --git a/drivers/gpu/drm/amd/pm/powerplay/hwmgr/smu7_hwmgr.c b/drivers/gpu/drm/amd/pm/powerplay/hwmgr/smu7_hwmgr.c
index 53849fd3615f..965ffcac17f8 100644
--- a/drivers/gpu/drm/amd/pm/powerplay/hwmgr/smu7_hwmgr.c
+++ b/drivers/gpu/drm/amd/pm/powerplay/hwmgr/smu7_hwmgr.c
@@ -5437,8 +5437,7 @@ static int smu7_get_thermal_temperature_range(struct pp_hwmgr *hwmgr,
 		thermal_data->max = table_info->cac_dtp_table->usSoftwareShutdownTemp *
 			PP_TEMPERATURE_UNITS_PER_CENTIGRADES;
 	else if (hwmgr->pp_table_version == PP_TABLE_V0)
-		thermal_data->max = data->thermal_temp_setting.temperature_shutdown *
-			PP_TEMPERATURE_UNITS_PER_CENTIGRADES;
+		thermal_data->max = data->thermal_temp_setting.temperature_shutdown;
 
 	thermal_data->sw_ctf_threshold = thermal_data->max;
 
diff --git a/drivers/gpu/drm/bridge/lontium-lt9211.c b/drivers/gpu/drm/bridge/lontium-lt9211.c
index 4d404f5ef87e..ea192c90b543 100644
--- a/drivers/gpu/drm/bridge/lontium-lt9211.c
+++ b/drivers/gpu/drm/bridge/lontium-lt9211.c
@@ -120,8 +120,7 @@ static int lt9211_read_chipid(struct lt9211 *ctx)
 	}
 
 	/* Test for known Chip ID. */
-	if (chipid[0] != REG_CHIPID0_VALUE || chipid[1] != REG_CHIPID1_VALUE ||
-	    chipid[2] != REG_CHIPID2_VALUE) {
+	if (chipid[0] != REG_CHIPID0_VALUE || chipid[1] != REG_CHIPID1_VALUE) {
 		dev_err(ctx->dev, "Unknown Chip ID: 0x%02x 0x%02x 0x%02x\n",
 			chipid[0], chipid[1], chipid[2]);
 		return -EINVAL;
diff --git a/drivers/gpu/drm/exynos/exynos7_drm_decon.c b/drivers/gpu/drm/exynos/exynos7_drm_decon.c
index 5f8e5e87d7cd..0ed62cd51fb5 100644
--- a/drivers/gpu/drm/exynos/exynos7_drm_decon.c
+++ b/drivers/gpu/drm/exynos/exynos7_drm_decon.c
@@ -51,7 +51,6 @@ struct decon_context {
 	void __iomem			*regs;
 	unsigned long			irq_flags;
 	bool				i80_if;
-	bool				suspended;
 	wait_queue_head_t		wait_vsync_queue;
 	atomic_t			wait_vsync_event;
 
@@ -81,13 +80,30 @@ static const enum drm_plane_type decon_win_types[WINDOWS_NR] = {
 	DRM_PLANE_TYPE_CURSOR,
 };
 
-static void decon_wait_for_vblank(struct exynos_drm_crtc *crtc)
+/**
+ * decon_shadow_protect_win() - disable updating values from shadow registers at vsync
+ *
+ * @ctx: display and enhancement controller context
+ * @win: window to protect registers for
+ * @protect: 1 to protect (disable updates)Linux 6.6.114Greg Kroah-Hartman <gregkh@linuxfoundation.org> undefinedlinux-kernel@vger.kernel.org, akpm@linux-foundation.org, torvalds@linux-foundation.org, stable@vger.kernel.org undefined undefined undefined undefined undefined undefined