mx6ul.dtsi | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/arch/arm/boot/dts/nxp/imx/imx6ul.dtsi b/arch/arm/boot/dts/nxp/imx/imx6ul.dtsi
index 6de224dd2bb9..6eb80f867f50 100644
--- a/arch/arm/boot/dts/nxp/imx/imx6ul.dtsi
+++ b/arch/arm/boot/dts/nxp/imx/imx6ul.dtsi
@@ -339,7 +339,7 @@ sai3: sai@2030000 {
 					#sound-dai-cells = <0>;
 					compatible = "fsl,imx6ul-sai", "fsl,imx6sx-sai";
 					reg = <0x02030000 0x4000>;
-					interrupts = <GIC_SPI 24 IRQ_TYPE_LEVEL_HIGH>;
+					interrupts = <GIC_SPI 25 IRQ_TYPE_LEVEL_HIGH>;
 					clocks = <&clks IMX6UL_CLK_SAI3_IPG>,
 						 <&clks IMX6UL_CLK_SAI3>,
 						 <&clks IMX6UL_CLK_DUMMY>, <&clks IMX6UL_CLK_DUMMY>;
-- 
2.51.0[PATCH] ARM: dts: nxp: imx6ul: correct SAI3 interrupt lineMaarten Zanders <maarten@zanders.be> undefinedRob Herring <robh@kernel.org>, Krzysztof Kozlowski <krzk+dt@kernel.org>, Conor Dooley <conor+dt@kernel.org>, Shawn Guo <shawnguo@kernel.org>, Sascha Hauer <s.hauer@pengutronix.de>, Pengutronix Kernel Team <kernel@pengutronix.de>, Fabio Estevam <festevam@gmail.com>, Lothar WaÃŸmann <LW@KARO-electronics.de> undefined undefined undefined undefined undefined undefined undefined undefined undefined undefined undefined undefined undefinedŠAƒÄ2
