al@kernel.org>
---
 drivers/net/wireless/realtek/rtw89/chan.c | 35 +++++++++++++++++++++++
 drivers/net/wireless/realtek/rtw89/chan.h |  2 ++
 drivers/net/wireless/realtek/rtw89/core.c |  2 ++
 drivers/net/wireless/realtek/rtw89/core.h |  2 ++
 4 files changed, 41 insertions(+)

diff --git a/drivers/net/wireless/realtek/rtw89/chan.c b/drivers/net/wireless/realtek/rtw89/chan.c
index b18019b53181c..17daf93fec0a4 100644
--- a/drivers/net/wireless/realtek/rtw89/chan.c
+++ b/drivers/net/wireless/realtek/rtw89/chan.c
@@ -1595,6 +1595,35 @@ static bool rtw89_mcc_duration_decision_on_bt(struct rtw89_dev *rtwdev)
 	return false;
 }
 
+void rtw89_mcc_prepare_done_work(struct wiphy *wiphy, struct wiphy_work *work)
+{
+	struct rtw89_dev *rtwdev = container_of(work, struct rtw89_dev,
+						mcc_prepare_done_work.work);
+
+	lockdep_assert_wiphy(wiphy);
+
+	ieee80211_wake_queues(rtwdev->hw);
+}
+
+static void rtw89_mcc_prepare(struct rtw89_dev *rtwdev, bool start)
+{
+	struct rtw89_mcc_info *mcc = &rtwdev->mcc;
+	struct rtw89_mcc_config *config = &mcc->config;
+
+	if (start) {
+		ieee80211_stop_queues(rtwdev->hw);
+
+		wiphy_delayed_work_queue(rtwdev->hw->wiphy,
+					 &rtwdev->mcc_prepare_done_work,
+					 usecs_to_jiffies(config->prepare_delay));
+	} else {
+		wiphy_delayed_work_queue(rtwdev->hw->wiphy,
+					 &rtwdev->mcc_prepare_done_work, 0);
+		wiphy_delayed_work_flush(rtwdev->hw->wiphy,
+					 &rtwdev->mcc_prepare_done_work);
+	}
+}
+
 static int rtw89_mcc_fill_start_tsf(struct rtw89_dev *rtwdev)
 {
 	struct rtw89_mcc_info *mcc = &rtwdev->mcc;
@@ -1630,6 +1659,8 @@ static int rtw89_mcc_fill_start_tsf(struct rtw89_dev *rtwdev)
 
 	config->start_tsf = start_tsf;
 	config->start_tsf_in_aux_domain = tsf_aux + start_tsf - tsf;
+	config->prepare_delay = start_tsf - tsf;
+
 	return 0;
 }
 
@@ -2219,6 +2250,8 @@ static int rtw89_mcc_start(struct rtw89_dev *rtwdev)
 	rtw89_chanctx_notify(rtwdev, RTW89_CHANCTX_STATE_MCC_START);
 
 	rtw89_mcc_start_beacon_noa(rtwdev);
+
+	rtw89_mcc_prepare(rtwdev, true);
 	return 0;
 }
 
@@ -2307,6 +2340,8 @@ static void rtw89_mcc_stop(struct rtw89_dev *rtwdev,
 	rtw89_chanctx_notify(rtwdev, RTW89_CHANCTX_STATE_MCC_STOP);
 
 	rtw89_mcc_stop_beacon_noa(rtwdev);
+
+	rtw89_mcc_prepare(rtwdev, false);
 }
 
 static int rtw89_mcc_update(struct rtw89_dev *rtwdev)
diff --git a/drivers/net/wireless/realtek/rtw89/chan.h b/drivers/net/wireless/realtek/rtw89/chan.h
index 2a25563593af9..be998fdd8724b 100644
--- a/drivers/net/wireless/realtek/rtw89/chan.h
+++ b/drivers/net/wireless/realtek/rtw89/chan.h
@@ -129,6 +129,8 @@ const struct rtw89_chan *__rtw89_mgnt_chan_get(struct rtw89_dev *rtwdev,
 #define rtw89_mgnt_chan_get(rtwdev, link_index) \
 	__rtw89_mgnt_chan_get(rtwdev, __func__, link_index)
 
+void rtw89_mcc_prepare_done_work(struct wiphy *wiphy, struct wiphy_work *work);
+
 int rtw89_chanctx_ops_add(struct rtw89_dev *rtwdev,
 			  struct ieee80211_chanctx_conf *ctx);
 void rtw89_chanctx_ops_remove(struct rtw89_dev *rtwdev,
diff --git a/drivers/net/wireless/realtek/rtw89/core.c b/drivers/net/wireless/realtek/rtw89/core.c
index 894ab7ab94ccb..0e4d5679e426c 100644
--- a/drivers/net/wireless/realtek/rtw89/core.c
+++ b/drivers/net/wireless/realtek/rtw89/core.c
@@ -4816,6 +4816,7 @@ void rtw89_core_stop(struct rtw89_dev *rtwdev)
 	wiphy_delayed_work_cancel(wiphy, &rtwdev->coex_bt_devinfo_work);
 	wiphy_delayed_work_cancel(wiphy, &rtwdev->coex_rfk_chk_work);
 	wiphy_delayed_work_cancel(wiphy, &rtwdev->cfo_track_work);
+	wiphy_delayed_work_cancel(wiphy, &rtwdev->mcc_prepare_done_work);
 	cancel_delayed_work_sync(&rtwdev->forbid_ba_work);
 	wiphy_delayed_work_cancel(wiphy, &rtwdev->antdiv_work);
 
@@ -5042,6 +5043,7 @@ int rtw89_core_init(struct rtw89_dev *rtwdev)
 	wiphy_delayed_work_init(&rtwdev->coex_bt_devinfo_work, rtw89_coex_bt_devinfo_work);
 	wiphy_delayed_work_init(&rtwdev->coex_rfk_chk_work, rtw89_coex_rfk_chk_work);
 	wiphy_delayed_work_init(&rtwdev->cfo_track_work, rtw89_phy_cfo_track_work);
+	wiphy_delayed_work_init(&rtwdev->mcc_prepare_done_work, rtw89_mcc_prepare_done_work);
 	INIT_DELAYED_WORK(&rtwdev->forbid_ba_work, rtw89_forbid_ba_work);
 	wiphy_delayed_work_init(&rtwdev->antdiv_work, rtw89_phy_antdiv_work);
 	rtwdev->txq_wq = alloc_workqueue("rtw89_tx_wq", WQ_UNBOUND | WQ_HIGHPRI, 0);
diff --git a/drivers/net/wireless/realtek/rtw89/core.h b/drivers/net/wireless/realtek/rtw89/core.h
index 1c8f3b9b7c4c6..f505fe6da4a24 100644
--- a/drivers/net/wireless/realtek/rtw89/core.h
+++ b/drivers/net/wireless/realtek/rtw89/core.h
@@ -5728,6 +5728,7 @@ struct rtw89_mcc_config {
 	struct rtw89_mcc_sync sync;
 	u64 start_tsf;
 	u64 start_tsf_in_aux_domain;
+	u64 prepare_delay;
 	u16 mcc_interval; /* TU */
 	u16 beacon_offset; /* TU */
 };
@@ -5858,6 +5859,7 @@ struct rtw89_dev {
 	struct wiphy_delayed_work coex_bt_devinfo_work;
 	struct wiphy_delayed_work coex_rfk_chk_work;
 	struct wiphy_delayed_work cfo_track_work;
+	struct wiphy_delayed_work mcc_prepare_done_work;
 	struct delayed_work forbid_ba_work;
 	struct wiphy_delayed_work antdiv_work;
 	struct rtw89_ppdu_sts_info ppdu_sts;
-- 
2.51.0[PATCH 6.16.y 1/2] wifi: rtw89: mcc: stop TX during MCC prepareSasha Levin <sashal@kernel.org> undefinedstable@vger.kernel.org undefined undefined undefinedƒ+ƒ€&
