sb-audio: Kill timer properly at
removal") patched a UAF issue caused by the error timer.

However, because the error timer kill added in this patch occurs after the
endpoint delete, a race condition to UAF still occurs, albeit rarely.

Additionally, since kill-cleanup for urb is also missing, freed memory can
be accessed in interrupt context related to urb, which can cause UAF.

Therefore, to prevent this, error timer and urb must be killed before
freeing the heap memory.

Cc: <stable@vger.kernel.org>
Reported-by: syzbot+f02665daa2abeef4a947@syzkaller.appspotmail.com
Closes: https://syzkaller.appspot.com/bug?extid=f02665daa2abeef4a947
Fixes: 0718a78f6a9f ("ALSA: usb-audio: Kill timer properly at removal")
Signed-off-by: Jeongjun Park <aha310510@gmail.com>
Signed-off-by: Takashi Iwai <tiwai@suse.de>
---
 sound/usb/midi.c | 9 ++++-----
 1 file changed, 4 insertions(+), 5 deletions(-)

diff --git a/sound/usb/midi.c b/sound/usb/midi.c
index c3de2b137435..461e183680da 100644
--- a/sound/usb/midi.c
+++ b/sound/usb/midi.c
@@ -1522,15 +1522,14 @@ static void snd_usbmidi_free(struct snd_usb_midi *umidi)
 {
 	int i;
 
+	if (!umidi->disconnected)
+		snd_usbmidi_disconnect(&umidi->list);
+
 	for (i = 0; i < MIDI_MAX_ENDPOINTS; ++i) {
 		struct snd_usb_midi_endpoint *ep = &umidi->endpoints[i];
-		if (ep->out)
-			snd_usbmidi_out_endpoint_delete(ep->out);
-		if (ep->in)
-			snd_usbmidi_in_endpoint_delete(ep->in);
+		kfree(ep->out);
 	}
 	mutex_destroy(&umidi->mutex);
-	timer_shutdown_sync(&umidi->error_timer);
 	kfree(umidi);
 }
 
--[PATCH 6.12.y 6.6.y 6.1.y 5.15.y 5.10.y 5.4.y] ALSA: usb-audio: fix race condition to UAF in snd_usbmidi_freeJeongjun Park <aha310510@gmail.com> undefinedstable@vger.kernel.org undefined undefined undefined undefined undefined undefined undefinedƒVƒ†