e *adev,
 		info->prot_read = protections & 0x8 ? true : false;
 		info->prot_write = protections & 0x10 ? true : false;
 		info->prot_exec = protections & 0x20 ? true : false;
-		mb();
-		atomic_set(&adev->gmc.vm_fault_info_updated, 1);
+		atomic_set_release(&adev->gmc.vm_fault_info_updated, 1);
 	}
 
 	return 0;
diff --git a/drivers/gpu/drm/amd/amdgpu/gmc_v8_0.c b/drivers/gpu/drm/amd/amdgpu/gmc_v8_0.c
index b45fa0cea9d2..0d4c93ff6f74 100644
--- a/drivers/gpu/drm/amd/amdgpu/gmc_v8_0.c
+++ b/drivers/gpu/drm/amd/amdgpu/gmc_v8_0.c
@@ -1179,7 +1179,7 @@ static int gmc_v8_0_sw_init(struct amdgpu_ip_block *ip_block)
 					GFP_KERNEL);
 	if (!adev->gmc.vm_fault_info)
 		return -ENOMEM;
-	atomic_set(&adev->gmc.vm_fault_info_updated, 0);
+	atomic_set_release(&adev->gmc.vm_fault_info_updated, 0);
 
 	return 0;
 }
@@ -1474,7 +1474,7 @@ static int gmc_v8_0_process_interrupt(struct amdgpu_device *adev,
 	vmid = REG_GET_FIELD(status, VM_CONTEXT1_PROTECTION_FAULT_STATUS,
 			     VMID);
 	if (amdgpu_amdkfd_is_kfd_vmid(adev, vmid)
-		&& !atomic_read(&adev->gmc.vm_fault_info_updated)) {
+		&& !atomic_read_acquire(&adev->gmc.vm_fault_info_updated)) {
 		struct kfd_vm_fault_info *info = adev->gmc.vm_fault_info;
 		u32 protections = REG_GET_FIELD(status,
 					VM_CONTEXT1_PROTECTION_FAULT_STATUS,
@@ -1490,8 +1490,7 @@ static int gmc_v8_0_process_interrupt(struct amdgpu_device *adev,
 		info->prot_read = protections & 0x8 ? true : false;
 		info->prot_write = protections & 0x10 ? true : false;
 		info->prot_exec = protections & 0x20 ? true : false;
-		mb();
-		atomic_set(&adev->gmc.vm_fault_info_updated, 1);
+		atomic_set_release(&adev->gmc.vm_fault_info_updated, 1);
 	}
 
 	return 0;
-- 
2.25.1[PATCH] drm/amdgpu: use atomic functions with memory barriers for vm fault infoGui-Dong Han <hanguidong02@gmail.com> undefinedFelix.Kuehling@amd.com, alexander.deucher@amd.com, christian.koenig@amd.com, airlied@gmail.com, simona@ffwll.ch undefined undefined undefined undefined undefined undefined undefined undefined undefined undefined„