ls = <31>;
+			num-channels = <23>;
 			interrupts = <GIC_SPI 164 IRQ_TYPE_LEVEL_HIGH>;
 			#dma-cells = <1>;
 			qcom,ee = <1>;
-			qcom,num-ees = <2>;
+			qcom,num-ees = <4>;
 			iommus = <&apps_smmu 0x1806 0x0>;
 		};
 FAILED: patch "[PATCH] arm64: dts: qcom: sdm845: Fix slimbam num-channels/ees" failed to apply to 5.15-stable tree<gregkh@linuxfoundation.org> undefinedstephan.gerhold@linaro.org,andersson@kernel.org,dmitry.baryshkov@oss.qualcomm.com undefined undefined undefined undefined”%ƒŸ0
