l.org>' --in-reply-to '2025101637-delegate-oversold-c71e@gregkh' --subject-prefix 'PATCH 6.17.y' HEAD^..

Possible dependencies:



thanks,

greg k-h

------------------ original commit in Linus's tree ------------------

From 6a5e9b9738a32229e2673d4eccfcbfe2ef3a1ab4 Mon Sep 17 00:00:00 2001
From: Viken Dadhaniya <viken.dadhaniya@oss.qualcomm.com>
Date: Mon, 30 Jun 2025 12:13:38 +0530
Subject: [PATCH] arm64: dts: qcom: qcs615: add missing dt property in QUP SEs

Add the missing required-opps and operating-points-v2 properties to
several I2C, SPI, and UART nodes in the QUP SEs.

Fixes: f6746dc9e379 ("arm64: dts: qcom: qcs615: Add QUPv3 configuration")
Cc: stable@vger.kernel.org
Signed-off-by: Viken Dadhaniya <viken.dadhaniya@oss.qualcomm.com>
Reviewed-by: Dmitry Baryshkov <dmitry.baryshkov@oss.qualcomm.com>
Link: https://lore.kernel.org/r/20250630064338.2487409-1-viken.dadhaniya@oss.qualcomm.com
Signed-off-by: Bjorn Andersson <andersson@kernel.org>

diff --git a/arch/arm64/boot/dts/qcom/sm6150.dtsi b/arch/arm64/boot/dts/qcom/sm6150.dtsi
index bfbb21035492..e033b53f0f0f 100644
--- a/arch/arm64/boot/dts/qcom/sm6150.dtsi
+++ b/arch/arm64/boot/dts/qcom/sm6150.dtsi
@@ -631,6 +631,7 @@ &mc_virt SLAVE_EBI1 QCOM_ICC_TAG_ALWAYS>,
 				interconnect-names = "qup-core",
 						     "qup-config";
 				power-domains = <&rpmhpd RPMHPD_CX>;
+				operating-points-v2 = <&qup_opp_table>;
 				status = "disabled";
 			};
 
@@ -654,6 +655,7 @@ &config_noc SLAVE_QUP_0 QCOM_ICC_TAG_ALWAYS>,
 						     "qup-config",
 						     "qup-memory";
 				power-domains = <&rpmhpd RPMHPD_CX>;
+				required-opps = <&rpmhpd_opp_low_svs>;
 				dmas = <&gpi_dma0 0 1 QCOM_GPI_I2C>,
 				       <&gpi_dma0 1 1 QCOM_GPI_I2C>;
 				dma-names = "tx",
@@ -681,6 +683,7 @@ &config_noc SLAVE_QUP_0 QCOM_ICC_TAG_ALWAYS>,
 						     "qup-config",
 						     "qup-memory";
 				power-domains = <&rpmhpd RPMHPD_CX>;
+				required-opps = <&rpmhpd_opp_low_svs>;
 				dmas = <&gpi_dma0 0 2 QCOM_GPI_I2C>,
 				       <&gpi_dma0 1 2 QCOM_GPI_I2C>;
 				dma-names = "tx",
@@ -703,6 +706,7 @@ &mc_virt SLAVE_EBI1 QCOM_ICC_TAG_ALWAYS>,
 				interconnect-names = "qup-core",
 						     "qup-config";
 				power-domains = <&rpmhpd RPMHPD_CX>;
+				operating-points-v2 = <&qup_opp_table>;
 				dmas = <&gpi_dma0 0 2 QCOM_GPI_SPI>,
 				       <&gpi_dma0 1 2 QCOM_GPI_SPI>;
 				dma-names = "tx",
@@ -728,6 +732,7 @@ &mc_virt SLAVE_EBI1 QCOM_ICC_TAG_ALWAYS>,
 				interconnect-names = "qup-core",
 						     "qup-config";
 				power-domains = <&rpmhpd RPMHPD_CX>;
+				operating-points-v2 = <&qup_opp_table>;
 				status = "disabled";
 			};
 
@@ -751,6 +756,7 @@ &config_noc SLAVE_QUP_0 QCOM_ICC_TAG_ALWAYS>,
 						     "qup-config",
 						     "qup-memory";
 				power-domains = <&rpmhpd RPMHPD_CX>;
+				required-opps = <&rpmhpd_opp_low_svs>;
 				dmas = <&gpi_dma0 0 3 QCOM_GPI_I2C>,
 				       <&gpi_dma0 1 3 QCOM_GPI_I2C>;
 				dma-names = "tx",FAILED: patch "[PATCH] arm64: dts: qcom: qcs615: add missing dt property in QUP SEs" failed to apply to 6.17-stable tree<gregkh@linuxfoundation.org> undefinedviken.dadhaniya@oss.qualcomm.com,andersson@kernel.org,dmitry.baryshkov@oss.qualcomm.com undefined undefined undefined undefined•-ƒŸ2
