= <950000 950000 950000>;
-			clock-latency-ns = <40000>;
-		};
 	};
 
 	gpu_opp_table: opp-table-gpu {

---
base-commit: ec714e371f22f716a04e6ecb2a24988c92b26911
change-id: 20251009-rk3576_opp-7bafcadef820

Best regards,
-- 
Alexey Charkov <alchark@gmail.com>[PATCH] arm64: dts: rockchip: Remove non-functioning CPU OPPs from RK3576Alexey Charkov <alchark@gmail.com> undefinedRob Herring <robh@kernel.org>, Krzysztof Kozlowski <krzk+dt@kernel.org>, Conor Dooley <conor+dt@kernel.org>, Heiko Stuebner <heiko@sntech.de>, Yifeng Zhao <yifeng.zhao@rock-chips.com>, Finley Xiao <finley.xiao@rock-chips.com>, Detlev Casanova <detlev.casanova@collabora.com>, Elaine Zhang <zhangqing@rock-chips.com>, Liang Chen <cl@rock-chips.com> undefined undefined undefined undefined undefined undefined undefined undefined undefined undefined undefined undefined undefined undefinedˆ`ƒ‰&
