ffline 16-31 no         yes

* Configure memory
echo 1 > /sys/firmware/memory/memory16/config
lsmem -o RANGE,SIZE,STATE,BLOCK,CONFIGURED,MEMMAP_ON_MEMORY
RANGE                  SIZE  STATE   BLOCK CONFIGURED MEMMAP_ON_MEMORY
0x00000000-0x7fffffff    2G  online  0-15  yes        no
0x80000000-0x87ffffff  128M offline    16  yes        yes
0x88000000-0xffffffff  1.9G offline 17-31  no         yes

* Deconfigure memory
echo 0 > /sys/firmware/memory/memory16/config
lsmem -o RANGE,SIZE,STATE,BLOCK,CONFIGURED,MEMMAP_ON_MEMORY
RANGE                 SIZE   STATE BLOCK CONFIGURED MEMMAP_ON_MEMORY
0x00000000-0x7fffffff   2G  online 0-15  yes        no
0x80000000-0xffffffff   2G offline 16-31 no         yes

* Enable memmap_on_memory and online it.
(Deconfigure first)
echo 0 > /sys/devices/system/memory/memory5/online
echo 0 > /sys/firmware/memory/memory5/config

lsmem -o RANGE,SIZE,STATE,BLOCK,CONFIGURED,MEMMAP_ON_MEMORY
RANGE                  SIZE  STATE  BLOCK CONFIGURED MEMMAP_ON_MEMORY
0x00000000-0x27ffffff  640M  online 0-4   yes        no
0x28000000-0x2fffffff  128M offline 5     no         no
0x30000000-0x7fffffff  1.3G  online 6-15  yes        no
0x80000000-0xffffffff    2G offline 16-31 no         yes

(Enable memmap_on_memory and online it)
echo 1 > /sys/firmware/memory/memory5/memmap_on_memory
echo 1 > /sys/firmware/memory/memory5/config
echo 1 > /sys/devices/system/memory/memory5/online

lsmem -o RANGE,SIZE,STATE,BLOCK,CONFIGURED,MEMMAP_ON_MEMORY
RANGE                  SIZE  STATE   BLOCK CONFIGURED MEMMAP_ON_MEMORY
0x00000000-0x27ffffff  640M  online  0-4   yes        no
0x28000000-0x2fffffff  128M  online  5     yes        yes
0x30000000-0x7fffffff  1.3G  online  6-15  yes        no
0x80000000-0xffffffff    2G  offline 16-31 no         yes

* Disable memmap_on_memory and online it.
(Deconfigure first)
echo 0 > /sys/devices/system/memory/memory5/online
echo 0 > /sys/firmware/memory/memory5/config

lsmem -o RANGE,SIZE,STATE,BLOCK,CONFIGURED,MEMMAP_ON_MEMORY
RANGE                  SIZE  STATE  BLOCK CONFIGURED MEMMAP_ON_MEMORY
0x00000000-0x27ffffff  640M  online 0-4   yes        no
0x28000000-0x2fffffff  128M offline 5     no         yes
0x30000000-0x7fffffff  1.3G  online 6-15  yes        no
0x80000000-0xffffffff    2G offline 16-31 no         yes

(Disable memmap_on_memory and online it)
echo 0 > /sys/firmware/memory/memory5/memmap_on_memory
echo 1 > /sys/firmware/memory/memory5/config
echo 1 > /sys/devices/system/memory/memory5/online

lsmem -o RANGE,SIZE,STATE,BLOCK,CONFIGURED,MEMMAP_ON_MEMORY
RANGE                  SIZE  STATE   BLOCK CONFIGURED MEMMAP_ON_MEMORY
0x00000000-0x7fffffff  2G    online  0-15  yes        no
0x80000000-0xffffffff  2G    offline 16-31 no         yes

* Userspace changes:
lsmem/chmem tool is also changed to use the new interface. I will send
it to util-linux soon.

Patch 1 adds support for removal of boot-allocated memory blocks.

Patch 2 provides option to dynamically configure and deconfigure memory
with/without memmap_on_memory.

Patch 3 removes MHP_OFFLINE_INACCESSIBLE from s390. The mhp flag was
used to mark memory as not accessible until memory hotplug online phase
begins.  However, with patch 2, it is no longer essential. Memory can be
brought to accessible state before adding memory, as the memory is added
during runttime now instead of boottime.

Patch 4 removes the MEM_PREPARE_ONLINE/MEM_FINISH_OFFLINE notifiers. It
is no longer needed.  Memory can be brought to accessible state before
adding memory now, with runtime (de)configuration of memory.

Note: The patches apply to the linux-next branch.

v3:
Thanks David
* Avoid goto label in create_standby_sclp_mems().
* Use unsigned long instead of u64.
* Add Acked-by.

v2:
Thanks David
* Rename struct mblock/mblock_arg with struct sclp_mem/sclp_mem_arg.
* Rename all mblocks/mblock references with sclp_mems/sclp_mem -
  structures, functions.
* Rename create_online_mblock() with create_configured_sclp_mem().
* Rename config_mblock_show()/config_mblock_store() with
  config_sclp_mem_show()/config_sclp_mem_store().
* Remove contains_standby_increment() and
  sclp_mem_notifier. sclp mem state change is performed when
  adding/removing memory. sclp memory notifier - no longer needed with
  this patchset.
* Recover sclp mem state when add_memory() fails.
* Refactor and add function init_sclp_mem().
* Use unsigned long instead of unsigned long long.
* Simplify and correct kobj handling. Thanks Heiko.

Sumanth Korikkar (4):
  s390/mm: Support removal of boot-allocated virtual memory map
  s390/sclp: Add support for dynamic (de)configuration of memory
  s390/sclp: Remove MHP_OFFLINE_INACCESSIBLE
  mm/memory_hotplug: Remove MEM_PREPARE_ONLINE/MEM_FINISH_OFFLINE
    notifiers

 arch/s390/mm/pgalloc.c         |   2 +
 arch/s390/mm/vmem.c            |  21 +--
 drivers/base/memory.c          |  23 +--
 drivers/s390/char/sclp_mem.c   | 288 +++++++++++++++++++++++----------
 include/linux/memory.h         |   9 --
 include/linux/memory_hotplug.h |  18 +--
 include/linux/memremap.h       |   1 -
 mm/memory_hotplug.c            |  17 +-
 mm/sparse.c                    |   3 +-
 9 files changed, 225 insertions(+), 157 deletions(-)

-- 
2.48.1[PATCH v3 0/4] Support dynamic (de)configuration of memorySumanth Korikkar <sumanthk@linux.ibm.com> undefinedAndrew Morton <akpm@linux-foundation.org>, David Hildenbrand <david@redhat.com>, linux-mm <linux-mm@kvack.org> undefined undefined undefined undefined undefined undefined undefined undefined undefined¾Cƒ‹c	