mis.org>
Signed-off-by: Thomas Gleixner <tglx@linutronix.de>
Tested-by: Guenter Roeck <linux@roeck-us.net>
Reviewed-by: Guenter Roeck <linux@roeck-us.net>
Reviewed-by: Jacob Keller <jacob.e.keller@intel.com>
Reviewed-by: Anna-Maria Behnsen <anna-maria@linutronix.de>
Link: https://lkml.kernel.org/r/20221106212702.182883323@goodmis.org
Link: https://lore.kernel.org/all/20221105060155.592778858@goodmis.org/
Link: https://lore.kernel.org/r/20221110064147.158230501@goodmis.org
Link: https://lore.kernel.org/r/20221123201624.634354813@linutronix.de
Signed-off-by: Jeongjun Park <aha310510@gmail.com>
---
 drivers/clocksource/timer-sp804.c | 6 +++---
 1 file changed, 3 insertions(+), 3 deletions(-)

diff --git a/drivers/clocksource/timer-sp804.c b/drivers/clocksource/timer-sp804.c
index e6a87f4af2b5..cd1916c05325 100644
--- a/drivers/clocksource/timer-sp804.c
+++ b/drivers/clocksource/timer-sp804.c
@@ -155,14 +155,14 @@ static irqreturn_t sp804_timer_interrupt(int irq, void *dev_id)
 	return IRQ_HANDLED;
 }
 
-static inline void timer_shutdown(struct clock_event_device *evt)
+static inline void evt_timer_shutdown(struct clock_event_device *evt)
 {
 	writel(0, common_clkevt->ctrl);
 }
 
 static int sp804_shutdown(struct clock_event_device *evt)
 {
-	timer_shutdown(evt);
+	evt_timer_shutdown(evt);
 	return 0;
 }
 
@@ -171,7 +171,7 @@ static int sp804_set_periodic(struct clock_event_device *evt)
 	unsigned long ctrl = TIMER_CTRL_32BIT | TIMER_CTRL_IE |
 			     TIMER_CTRL_PERIODIC | TIMER_CTRL_ENABLE;
 
-	timer_shutdown(evt);
+	evt_timer_shutdown(evt);
 	writel(common_clkevt->reload, common_clkevt->load);
 	writel(ctrl, common_clkevt->ctrl);
 	return 0;
--[PATCH 6.1.y 04/12] clocksource/drivers/sp804: Do not use timer namespace for timer_shutdown() functionJeongjun Park <aha310510@gmail.com> undefinedstable@vger.kernel.org undefined undefined undefined undefined undefined undefined undefined undefined undefined undefined undefined undefined undefined undefined undefined undefined undefined undefined‘