the address, and the 'd's are
    the decimal values of the four low-order 8-bit pieces of the
    address (standard IPv4 representation) as defined in RFC 4291 2.2 p.3.

z0Can not apply to non-IPv4-mapped IPv6 address %sr