# master 2

canonical_ip: 10.153.7.111

interface_bonding:
    name: bond0
    members:
        - ens9f1
        - ens9f2
    mode: 802.3ad
    miimon: 100

interface_IPs:
    baremetal:
        description: "OCP Baremetal Network"
        interface_name: "baremetal"
        interface: bond0
        vlan: 1182
        ipv4: 10.153.11.111/24

    outside:
        description: "OSP Provider Network"
        interface_name: "baremetal"
        interface: bond0
        vlan: 1183
        ipv4: 10.153.12.111/24

    pxe:
        description: "PXE Boot Network"
        interface_name: "pxe"
        interface: bond0
        macaddress: 84:16:0C:AE:52:DF
        vlan: 1184

    storage:
        description: "Storage Network"
        interface_name: "storage"
        interface: bond0
        vlan: 1198
        ipv4: 10.153.40.111/24

ipmi:
    ip_address: 192.168.208.151

root_device: /dev/nvme0n1
