# master 0 

canonical_ip: 10.153.7.109

interface_bonding:
  name: bond0
  members:
    - ens6f0np0
    - ens6f1np1
  mode: 802.3ad
  miimon: 100

interface_IPs:
  baremetal:
    description: "OCP Baremetal Network"
    interface_name: "baremetal"
    interface: bond0
    vlan: 1182
    ipv4: 10.153.11.109/24

  outside:
    description: "OSP Provider Network"
    interface_name: "baremetal"
    interface: bond0
    vlan: 1183
    ipv4: 10.153.6.109/24

  pxe:
    description: "PXE Boot Network"
    interface_name: "pxe"
    interface: bond0
    macaddress: E4:3D:1A:62:FB:AB
    vlan: 1184

  storage:
    description: "Storage Network"
    interface_name: "storage"
    interface: bond0
    vlan: "1201"
    ipv4: 10.153.48.109/24

ipmi:
  ip_address: 192.168.208.149

root_device: /dev/nvme0n1
