# osp node 2

canonical_ip: 10.153.7.113

interface_bonding:
    name: bond0
    members:
        - ens9f1
        - ens9f2
    mode: 802.3ad
    miimon: 100

interface_IPs:
    ctlplane:
        description: "OSP Controlplane Network"
        interface_name: "ctlplane"
        interface: bond0
        vlan: 1179
        ipv4: 10.153.8.113/24

    tenant:
        description: "OSP Tenant Network"
        interface_name: "tenant"
        interface: bond0
        vlan: 1180
        ipv4: 10.153.9.113/24

    intapi:
        description: "OSP Internal API Network"
        interface_name: "intapi"
        interface: bond0
        vlan: 1181
        ipv4: 10.153.10.113/24

    outside:
        description: "OSP Provider Network"
        interface_name: "provider"
        interface: bond0
        vlan: 1183
        ipv4: 10.153.12.113/24

    pxe:
        description: "PXE Boot Network"
        interface_name: "pxe"
        interface: bond0
        vlan: 1184
        ipv4: 10.153.15.113/24

    storage:
        description: "Storage Network"
        interface_name: "storage"
        interface: bond0
        vlan: 1198
        ipv4: 10.153.40.113/24

ipmi:
    ip_address: 192.168.208.153

root_device: /dev/nvme0n1
