# Usecase for device HDMI1/Display Port stereo playback on Intel SKYLAKE/KABYLAKE platforms
# For Audio in I2S mode

SectionDevice."Hdmi1" {
        Comment "HDMI/Display Port 1 Stereo"

        EnableSequence [
                exec "echo Hdmi1 EnableSequnece"
        ]

        DisableSequence [
                exec "echo Hdmi1 DisableSequnece"
        ]

        Value {
                PlaybackPCM "hw:broxtonrt298,4"
                PlaybackChannels "2"
                PlaybackPriority "3"
                JackControl "HDMI/DP, pcm=4 Jack"
        }
}

