#
#  ALSA library configuration file
#

# pre-load the configuration files

@hooks [
	{
		func load
		files [
			"/usr/etc/alsa/conf.d"
			"/etc/alsa/conf.d"
			"/etc/asound.conf|||/usr/etc/asound.conf"
			"~/.asoundrc"
			{
				@func concat
				strings [
					{
						@func getenv
						vars [
							XDG_CONFIG_HOME
						]
						default "~/.config"
					}
					"/alsa/asoundrc"
				]
			}
		]
		errors false
	}
]

# load card-specific configuration files (on request)

cards.@hooks [
	{
		func load
		files [
			{
				@func concat
				strings [
					{ @func datadir }
					"/cards/aliases.conf"
				]
			}
		]
	}
	{
		func load_for_all_cards
		files [
			{
				@func concat
				strings [
					{ @func datadir }
					"/cards/"
					{ @func private_string }
					".conf"
				]
			}
		]
		errors false
	}
]

#
# defaults
#

# show all name hints also for definitions without hint {} section
defaults.namehint.showall on
# show just basic name hints
defaults.namehint.basic on
# show extended name hints
defaults.namehint.extended on
#
defaults.ctl.card 0
defaults.pcm.card 0
defaults.pcm.device 0
defaults.pcm.subdevice -1
defaults.pcm.nonblock 1
defaults.pcm.compat 0
defaults.pcm.minperiodtime 5000		# in us
defaults.pcm.ipc_key 5678293
defaults.pcm.ipc_gid audio
defaults.pcm.ipc_perm 0660
defaults.pcm.tstamp_type default
defaults.pcm.dmix.max_periods 0
defaults.pcm.dmix.channels 2
defaults.pcm.dmix.rate 48000
defaults.pcm.dmix.format unchanged
defaults.pcm.dmix.card defaults.pcm.card
defaults.pcm.dmix.device defaults.pcm.device
defaults.pcm.dsnoop.card defaults.pcm.card
defaults.pcm.dsnoop.device defaults.pcm.device
defaults.pcm.front.card defaults.pcm.card
defaults.pcm.front.device defaults.pcm.device
defaults.pcm.rear.card defaults.pcm.card
defaults.pcm.rear.device defaults.pcm.device
defaults.pcm.center_lfe.card defaults.pcm.card
defaults.pcm.center_lfe.device defaults.pcm.device
defaults.pcm.side.card defaults.pcm.card
defaults.pcm.side.device defaults.pcm.device
defaults.pcm.surround21.card defaults.pcm.card
defaults.pcm.surround21.device defaults.pcm.device
defaults.pcm.surround40.card defaults.pcm.card
defaults.pcm.surround40.device defaults.pcm.device
defaults.pcm.surround41.card defaults.pcm.card
defaults.pcm.surround41.device defaults.pcm.device
defaults.pcm.surround50.card defaults.pcm.card
defaults.pcm.surround50.device defaults.pcm.device
defaults.pcm.surround51.card defaults.pcm.card
defaults.pcm.surround51.device defaults.pcm.device
defaults.pcm.surround71.card defaults.pcm.card
defaults.pcm.surround71.device defaults.pcm.device
defaults.pcm.iec958.card defaults.pcm.card
defaults.pcm.iec958.device defaults.pcm.device
defaults.pcm.modem.card defaults.pcm.card
defaults.pcm.modem.device defaults.pcm.device
defaults.pcm.file_format raw
defaults.pcm.file_truncate true		# truncate files via file or tee PCM
defaults.rawmidi.card 0
defaults.rawmidi.device 0
defaults.rawmidi.subdevice -1
defaults.hwdep.card 0
defaults.hwdep.device 0
defaults.timer.class 2
defaults.timer.sclass 0
defaults.timer.card 0
defaults.timer.device 0
defaults.timer.subdevice 0

#
#  PCM interface
#

pcm.hw {
	@args [ CARD DEV SUBDEV ]
	@args.CARD {
		type string
		default {
			@func getenv
			vars [
				ALSA_PCM_CARD
				ALSA_CARD
			]
			default {
				@func refer
				name defaults.pcm.card
			}
		}
	}
	@args.DEV {
		type integer
		default {
			@func igetenv
			vars [
				ALSA_PCM_DEVICE
			]
			default {
				@func refer
				name defaults.pcm.device
			}
		}
	}
	@args.SUBDEV {
		type integer
		default {
			@func refer
			name defaults.pcm.subdevice
		}
	}		
	type hw
	card $CARD
	device $DEV
	subdevice $SUBDEV
	hint {
		show {
			@func refer
			name defaults.namehint.extended
		}
		description "Direct hardware device without any conversions"
	}
}

pcm.plughw {
	@args [ CARD DEV SUBDEV ]
	@args.CARD {
		type string
		default {
			@func getenv
			vars [
				ALSA_PCM_CARD
				ALSA_CARD
			]
			default {
				@func refer
				name defaults.pcm.card
			}
		}
	}
	@args.DEV {
		type integer
		default {
			@func igetenv
			vars [
				ALSA_PCM_DEVICE
			]
			default {
				@func refer
				name defaults.pcm.device
			}
		}
	}
	@args.SUBDEV {
		type integer
		default {
			@func refer
			name defaults.pcm.subdevice
		}
	}		
	type plug
	slave.pcm {
		type hw
		card $CARD
		device $DEV
		subdevice $SUBDEV
	}
	hint {
		show {
			@func refer
			name defaults.namehint.extended
		}
		description "Hardware device with all software conversions"
	}
}

pcm.plug {
	@args [ SLAVE ]
	@args.SLAVE {
		type string
	}
	type plug
	slave.pcm $SLAVE
}

pcm.shm {
	@args [ SOCKET PCM ]
	@args.SOCKET {
		type string
	}
	@args.PCM {
		type string
	}
	type shm
	server $SOCKET
	pcm $PCM
}

pcm.tee {
	@args [ SLAVE FILE FORMAT ]
	@args.SLAVE {
		type string
	}
	@args.FILE {
		type string
	}
	@args.FORMAT {
		type string
		default {
			@func refer
			name defaults.pcm.file_format
		}
	}
	type file
	slave.pcm $SLAVE
	file $FILE
	format $FORMAT
	truncate {
		@func refer
		name defaults.pcm.file_truncate
	}
}

pcm.file {
	@args [ FILE FORMAT ]
	@args.FILE {
		type string
	}
	@args.FORMAT {
		type string
		default {
			@func refer
			name defaults.pcm.file_format
		}
	}
	type file
	slave.pcm null
	file $FILE
	format $FORMAT
	truncate {
		@func refer
		name defaults.pcm.file_truncate
	}
}

pcm.null {
	type null
	hint {
		show {
			@func refer
			name defaults.namehint.basic
		}
		description "Discard all samples (playback) or generate zero samples (capture)"
	}
}

# redirect to load-on-demand extended pcm definitions
pcm.cards cards.pcm

pcm.default cards.pcm.default
pcm.sysdefault cards.pcm.default
pcm.front cards.pcm.front
pcm.rear cards.pcm.rear
pcm.center_lfe cards.pcm.center_lfe
pcm.side cards.pcm.side
pcm.surround21 cards.pcm.surround21
pcm.surround40 cards.pcm.surround40
pcm.surround41 cards.pcm.surround41
pcm.surround50 cards.pcm.surround50
pcm.surround51 cards.pcm.surround51
pcm.surround71 cards.pcm.surround71
pcm.iec958 cards.pcm.iec958
pcm.spdif iec958
pcm.hdmi cards.pcm.hdmi
pcm.dmix cards.pcm.dmix
pcm.dsnoop cards.pcm.dsnoop
pcm.modem cards.pcm.modem
pcm.phoneline cards.pcm.phoneline

#
#  Control interface
#
	
ctl.sysdefault {
	type hw
	card {
		@func getenv
		vars [
			ALSA_CTL_CARD
			ALSA_CARD
		]
		default {
			@func refer
			name defaults.ctl.card
		}
	}
	hint.description "Default control device"
}
ctl.default ctl.sysdefault

ctl.hw {
	@args [ CARD ]
	@args.CARD {
		type string
		default {
			@func getenv
			vars [
				ALSA_CTL_CARD
				ALSA_CARD
			]
			default {
				@func refer
				name defaults.ctl.card
			}
		}
	}
	type hw
	card $CARD
	hint.description "Direct control device"
}

ctl.shm {
	@args [ SOCKET CTL ]
	@args.SOCKET {
		type string
	}
	@args.CTL {
		type string
	}
	type shm
	server $SOCKET
	ctl $CTL
}

#
#  RawMidi interface
#

rawmidi.default {
	type hw
	card {
		@func getenv
		vars [
			ALSA_RAWMIDI_CARD
			ALSA_CARD
		]
		default {
			@func refer
			name defaults.rawmidi.card
		}
	}
	device {
		@func igetenv
		vars [
			ALSA_RAWMIDI_DEVICE
		]
		default {
			@func refer
			name defaults.rawmidi.device
		}
	}
	hint.description "Default raw MIDI device"
}

rawmidi.hw {
	@args [ CARD DEV SUBDEV ]
	@args.CARD {
		type string
		default {
			@func getenv
			vars [
				ALSA_RAWMIDI_CARD
				ALSA_CARD
			]
			default {
				@func refer
				name defaults.rawmidi.card
			}
		}
	}
	@args.DEV {
		type integer
		default {
			@func igetenv
			vars [
				ALSA_RAWMIDI_DEVICE
			]
			default {
				@func refer
				name defaults.rawmidi.device
			}
		}
	}
	@args.SUBDEV {
		type integer
		default -1
	}
	type hw
	card $CARD
	device $DEV
	subdevice $SUBDEV
	hint {
		description "Direct rawmidi driver device"
		device $DEV
	}
}

rawmidi.virtual {
	@args [ MERGE ]
	@args.MERGE {
		type string
		default 1
	}
	type virtual
	merge $MERGE
}

#
#  Sequencer interface
#

seq.default {
	type hw
	hint.description "Default sequencer device"
}

seq.hw {
	type hw
}

#
#  HwDep interface
#

hwdep.default {
	type hw
	card {
		@func getenv
		vars [
			ALSA_HWDEP_CARD
			ALSA_CARD
		]
		default {
			@func refer
			name defaults.hwdep.card
		}
	}
	device {
		@func igetenv
		vars [
			ALSA_HWDEP_DEVICE
		]
		default {
			@func refer
			name defaults.hwdep.device
		}
	}
	hint.description "Default hardware dependent device"
}

hwdep.hw {
	@args [ CARD DEV ]
	@args.CARD {
		type string
		default {
			@func getenv
			vars [
				ALSA_HWDEP_CARD
				ALSA_CARD
			]
			default {
				@func refer
				name defaults.hwdep.card
			}
		}
	}
	@args.DEV {
		type integer
		default {
			@func igetenv
			vars [
				ALSA_HWDEP_DEVICE
			]
			default {
				@func refer
				name defaults.hwdep.device
			}
		}
	}
	type hw
	card $CARD
	device $DEV
	hint {
		description "Direct hardware dependent device"
		device $DEV
	}
}

#
#  Timer interface
#

timer_query.default {
	type hw
}

timer_query.hw {
	type hw
}

timer.default {
	type hw
	class {
		@func refer
		name defaults.timer.class
	}
	sclass {
		@func refer
		name defaults.timer.sclass
	}
	card {
		@func refer
		name defaults.timer.card
	}
	device {
		@func refer
		name defaults.timer.device
	}
	subdevice {
		@func refer
		name defaults.timer.subdevice
	}
	hint.description "Default timer device"
}

timer.hw {
	@args [ CLASS SCLASS CARD DEV SUBDEV ]
	@args.CLASS {
		type integer
		default {
			@func refer
			name defaults.timer.class
		}
	}
	@args.SCLASS {
		type integer
		default {
			@func refer
			name defaults.timer.sclass
		}
	}
	@args.CARD {
		type string
		default {
			@func refer
			name defaults.timer.card
		}
	}
	@args.DEV {
		type integer
		default {
			@func refer
			name defaults.timer.device
		}
	}
	@args.SUBDEV {
		type integer
		default {
			@func refer
			name defaults.timer.subdevice
		}
	}
	type hw
	class $CLASS
	sclass $SCLASS
	card $CARD
	device $DEV
	subdevice $SUBDEV
	hint {
		description "Direct timer device"
		device $DEV
	}
}
