
.TH "GCLOUD_AI_TENSORBOARDS_UPDATE" 1



.SH "NAME"
.HP
gcloud ai tensorboards update \- update an existing Vertex AI Tensorboard



.SH "SYNOPSIS"
.HP
\f5gcloud ai tensorboards update\fR (\fITENSORBOARD\fR\ :\ \fB\-\-region\fR=\fIREGION\fR) [\fB\-\-description\fR=\fIDESCRIPTION\fR] [\fB\-\-display\-name\fR=\fIDISPLAY_NAME\fR] [\fB\-\-update\-labels\fR=[\fIKEY\fR=\fIVALUE\fR,...]] [\fB\-\-clear\-labels\fR\ |\ \fB\-\-remove\-labels\fR=[\fIKEY\fR,...]] [\fIGCLOUD_WIDE_FLAG\ ...\fR]



.SH "DESCRIPTION"

Update an existing Vertex AI Tensorboard.



.SH "EXAMPLES"

To update a Tensorboard \f512345\fR, in region \f5us\-central1\fR and project
\f5my\-project\fR, with the display name \f5updated display name\fR:

.RS 2m
$ gcloud ai tensorboards update \e
  projects/my\-project/locations/us\-central1/tensorboards/12345 \e
  \-\-display\-name="updated display name"
.RE



.SH "POSITIONAL ARGUMENTS"

.RS 2m
.TP 2m

Tensorboard resource \- The tensorboard to update. The arguments in this group
can be used to specify the attributes of this resource. (NOTE) Some attributes
are not given arguments in this group but can be set in other ways.

To set the \f5project\fR attribute:
.RS 2m
.IP "\(em" 2m
provide the argument \f5tensorboard\fR on the command line with a fully
specified name;
.IP "\(em" 2m
provide the argument \f5\-\-project\fR on the command line;
.IP "\(em" 2m
set the property \f5core/project\fR.
.RE
.sp

This must be specified.


.RS 2m
.TP 2m
\fITENSORBOARD\fR

ID of the tensorboard or fully qualified identifier for the tensorboard.

To set the \f5name\fR attribute:
.RS 2m
.IP "\(bu" 2m
provide the argument \f5tensorboard\fR on the command line.
.RE
.sp

This positional argument must be specified if any of the other arguments in this
group are specified.

.TP 2m
\fB\-\-region\fR=\fIREGION\fR

Cloud region for the tensorboard.

To set the \f5region\fR attribute:
.RS 2m
.IP "\(bu" 2m
provide the argument \f5tensorboard\fR on the command line with a fully
specified name;
.IP "\(bu" 2m
provide the argument \f5\-\-region\fR on the command line;
.IP "\(bu" 2m
set the property \f5ai/region\fR;
.IP "\(bu" 2m
choose one from the prompted list of available regions.
.RE
.sp


.RE
.RE
.sp

.SH "FLAGS"

.RS 2m
.TP 2m
\fB\-\-description\fR=\fIDESCRIPTION\fR

Description of the tensorboard.

.TP 2m
\fB\-\-display\-name\fR=\fIDISPLAY_NAME\fR

Display name of the tensorboard.

.TP 2m
\fB\-\-update\-labels\fR=[\fIKEY\fR=\fIVALUE\fR,...]

List of label KEY=VALUE pairs to update. If a label exists, its value is
modified. Otherwise, a new label is created.

Keys must start with a lowercase character and contain only hyphens (\f5\-\fR),
underscores (\f5_\fR), lowercase characters, and numbers. Values must contain
only hyphens (\f5\-\fR), underscores (\f5_\fR), lowercase characters, and
numbers.

.TP 2m

At most one of these can be specified:


.RS 2m
.TP 2m
\fB\-\-clear\-labels\fR

Remove all labels. If \f5\-\-update\-labels\fR is also specified then
\f5\-\-clear\-labels\fR is applied first.

For example, to remove all labels:

.RS 2m
$ gcloud ai tensorboards update \-\-clear\-labels
.RE

To remove all existing labels and create two new labels, \f5\fIfoo\fR\fR and
\f5\fIbaz\fR\fR:

.RS 2m
$ gcloud ai tensorboards update \-\-clear\-labels \e
  \-\-update\-labels foo=bar,baz=qux
.RE

.TP 2m
\fB\-\-remove\-labels\fR=[\fIKEY\fR,...]

List of label keys to remove. If a label does not exist it is silently ignored.
If \f5\-\-update\-labels\fR is also specified then \f5\-\-update\-labels\fR is
applied first.


.RE
.RE
.sp

.SH "GCLOUD WIDE FLAGS"

These flags are available to all commands: \-\-access\-token\-file, \-\-account,
\-\-billing\-project, \-\-configuration, \-\-flags\-file, \-\-flatten,
\-\-format, \-\-help, \-\-impersonate\-service\-account, \-\-log\-http,
\-\-project, \-\-quiet, \-\-trace\-token, \-\-user\-output\-enabled,
\-\-verbosity.

Run \fB$ gcloud help\fR for details.



.SH "NOTES"

These variants are also available:

.RS 2m
$ gcloud alpha ai tensorboards update
.RE

.RS 2m
$ gcloud beta ai tensorboards update
.RE


