{
  "schema_version": "1.4.0",
  "id": "GHSA-5cw5-jwpw-v565",
  "modified": "2022-05-17T01:25:01Z",
  "published": "2022-05-17T01:25:01Z",
  "aliases": [
    "CVE-2014-3335"
  ],
  "details": "Cisco IOS XR 4.3(.2) and earlier on ASR 9000 devices does not properly perform NetFlow sampling of packets with multicast destination MAC addresses, which allows remote attackers to cause a denial of service (chip and card hangs) via a crafted packet, aka Bug ID CSCup77750.",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2014-3335"
    },
    {
      "type": "WEB",
      "url": "https://exchange.xforce.ibmcloud.com/vulnerabilities/95443"
    },
    {
      "type": "WEB",
      "url": "http://secunia.com/advisories/60222"
    },
    {
      "type": "WEB",
      "url": "http://tools.cisco.com/security/center/content/CiscoSecurityNotice/CVE-2014-3335"
    },
    {
      "type": "WEB",
      "url": "http://tools.cisco.com/security/center/viewAlert.x?alertId=35416"
    },
    {
      "type": "WEB",
      "url": "http://www.securityfocus.com/bid/69383"
    },
    {
      "type": "WEB",
      "url": "http://www.securitytracker.com/id/1030757"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-20"
    ],
    "severity": "MODERATE",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2014-08-26T10:55:00Z"
  }
}