{
  "schema_version": "1.4.0",
  "id": "GHSA-5c4m-rpq3-mxjc",
  "modified": "2022-05-24T17:32:48Z",
  "published": "2022-05-24T17:32:48Z",
  "aliases": [
    "CVE-2020-11114"
  ],
  "details": "u'Bluetooth devices does not properly restrict the L2CAP payload length allowing users in radio range to cause a buffer overflow via a crafted Link Layer packet(Equivalent to CVE-2019-17060,CVE-2019-17061 and CVE-2019-17517 in Sweyntooth paper)' in Snapdragon Compute, Snapdragon Consumer IOT, Snapdragon Industrial IOT, Snapdragon IoT, Snapdragon Mobile, Snapdragon Voice & Music in AR9344",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2020-11114"
    },
    {
      "type": "WEB",
      "url": "https://www.qualcomm.com/company/product-security/bulletins/october-2020-bulletin"
    },
    {
      "type": "WEB",
      "url": "https://www.qualcomm.com/company/product-security/bulletins/october-2020-security-bulletin"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-125"
    ],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2020-11-02T07:15:00Z"
  }
}