{
  "schema_version": "1.4.0",
  "id": "GHSA-5f4r-g29m-jw8q",
  "modified": "2022-05-13T01:10:26Z",
  "published": "2022-05-13T01:10:26Z",
  "aliases": [
    "CVE-2017-18347"
  ],
  "details": "Incorrect access control in RDP Level 1 on STMicroelectronics STM32F0 series devices allows physically present attackers to extract the device's protected firmware via a special sequence of Serial Wire Debug (SWD) commands because there is a race condition between full initialization of the SWD interface and the setup of flash protection.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.1/AV:P/AC:L/PR:N/UI:N/S:U/C:H/I:N/A:N"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2017-18347"
    },
    {
      "type": "WEB",
      "url": "https://community.st.com/s/question/0D50X00009Xke7aSAB/readout-protection-cracked-on-stm32"
    },
    {
      "type": "WEB",
      "url": "https://www.aisec.fraunhofer.de/en/FirmwareProtection.html"
    },
    {
      "type": "WEB",
      "url": "https://www.usenix.org/conference/woot17/workshop-program/presentation/obermaier"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-362"
    ],
    "severity": "MODERATE",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2018-09-12T15:29:00Z"
  }
}