{
  "schema_version": "1.4.0",
  "id": "GHSA-5fvv-3p43-q895",
  "modified": "2022-05-14T03:35:05Z",
  "published": "2022-05-14T03:35:05Z",
  "aliases": [
    "CVE-2017-17282"
  ],
  "details": "SCCP (Signalling Connection Control Part) module in Huawei DP300 V500R002C00, RP200 V500R002C00, V600R006C00, TE30 V100R001C10, V500R002C00, V600R006C00, TE40 V500R002C00, V600R006C00, TE50 V500R002C00, V600R006C00, TE60 V100R001C10, V500R002C00, V600R006C00 has a buffer overflow vulnerability. An attacker has to find a way to send malformed packets to the affected products repeatedly. Due to insufficient input validation, successful exploit may cause some service abnormal.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.0/AV:A/AC:H/PR:N/UI:N/S:U/C:N/I:N/A:L"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2017-17282"
    },
    {
      "type": "WEB",
      "url": "http://www.huawei.com/en/psirt/security-advisories/huawei-sa-20180228-01-sccp-en"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-119"
    ],
    "severity": "LOW",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2018-03-09T21:29:00Z"
  }
}