{
  "schema_version": "1.4.0",
  "id": "GHSA-5f5q-pmvm-52cw",
  "modified": "2024-04-04T01:20:02Z",
  "published": "2022-05-24T16:50:52Z",
  "aliases": [
    "CVE-2019-2264"
  ],
  "details": "Null pointer dereference occurs for channel context while opening glink channel in Snapdragon Auto, Snapdragon Consumer IOT, Snapdragon Mobile, Snapdragon Voice & Music, Snapdragon Wearables in MDM9607, MDM9640, MSM8909W, QCS405, QCS605, SD 425, SD 427, SD 430, SD 435, SD 439 / SD 429, SD 450, SD 625, SD 632, SD 636, SD 712 / SD 710 / SD 670, SD 820A, SD 835, SD 845 / SD 850, SDM439, SDM630, SDM660, SDX24",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.0/AV:L/AC:L/PR:L/UI:N/S:U/C:H/I:H/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2019-2264"
    },
    {
      "type": "WEB",
      "url": "https://www.codeaurora.org/security-bulletin/2019/06/03/june-2019-code-aurora-security-bulletin"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-416"
    ],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2019-07-22T14:15:00Z"
  }
}