{
  "schema_version": "1.4.0",
  "id": "GHSA-5fh3-4cph-hp6v",
  "modified": "2022-05-13T01:46:58Z",
  "published": "2022-05-13T01:46:58Z",
  "aliases": [
    "CVE-2017-7450"
  ],
  "details": "AIRTAME HDMI dongle with firmware before 2.2.0 allows unauthenticated access to a big part of the management interface. It is possible to extract all information including the Wi-Fi password, reboot, or force a software update at an arbitrary time.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.0/AV:N/AC:L/PR:N/UI:N/S:U/C:H/I:H/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2017-7450"
    },
    {
      "type": "WEB",
      "url": "http://cweiske.de/tagebuch/airtame-security.htm"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-287"
    ],
    "severity": "CRITICAL",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2017-04-05T23:59:00Z"
  }
}