{
  "schema_version": "1.4.0",
  "id": "GHSA-7v3q-v7jh-m6pv",
  "modified": "2022-05-24T17:20:30Z",
  "published": "2022-05-24T17:20:30Z",
  "aliases": [
    "CVE-2020-14074"
  ],
  "details": "TRENDnet TEW-827DRU devices through 2.06B04 contain a stack-based buffer overflow in the ssi binary. The overflow allows an authenticated user to execute arbitrary code by POSTing to apply.cgi via the action kick_ban_wifi_mac_allow with a sufficiently long qcawifi.wifi0_vap0.maclist key.",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2020-14074"
    },
    {
      "type": "WEB",
      "url": "https://github.com/kuc001/IoTFirmware/blob/master/Trendnet/TEW-827/TRENDnet-kick_ban_wifi.pdf"
    },
    {
      "type": "WEB",
      "url": "https://github.com/kuc001/IoTFirmware/blob/master/Trendnet/TEW-827/kick_ban_wifi_mac_allow_overflow.pdf"
    }
  ],
  "database_specific": {
    "cwe_ids": [],
    "severity": "MODERATE",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2020-06-15T04:15:00Z"
  }
}