{
  "schema_version": "1.4.0",
  "id": "GHSA-7qxm-j3q6-829g",
  "modified": "2022-05-14T02:03:46Z",
  "published": "2022-05-14T02:03:46Z",
  "aliases": [
    "CVE-2015-6485"
  ],
  "details": "Schneider Electric Telvent Sage 2300 RTUs with firmware before C3413-500-S01, and LANDAC II-2, Sage 1410, Sage 1430, Sage 1450, Sage 2400, and Sage 3030M RTUs with firmware before C3414-500-S02J2, allow remote attackers to obtain sensitive information from device memory by reading a padding field of an Ethernet packet.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.0/AV:N/AC:L/PR:N/UI:N/S:U/C:L/I:N/A:N"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2015-6485"
    },
    {
      "type": "WEB",
      "url": "https://ics-cert.us-cert.gov/advisories/ICSA-16-070-01"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-200"
    ],
    "severity": "MODERATE",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2016-03-12T02:59:00Z"
  }
}