{
  "schema_version": "1.4.0",
  "id": "GHSA-9qwj-267h-cmr3",
  "modified": "2022-05-24T17:32:49Z",
  "published": "2022-05-24T17:32:49Z",
  "aliases": [
    "CVE-2020-11125"
  ],
  "details": "u'Out of bound access can happen in MHI command process due to lack of check of channel id value received from MHI devices' in Snapdragon Auto, Snapdragon Compute, Snapdragon Connectivity, Snapdragon Consumer IOT, Snapdragon Industrial IOT, Snapdragon Mobile, Snapdragon Voice & Music, Snapdragon Wearables, Snapdragon Wired Infrastructure and Networking in Agatti, APQ8009, Bitra, IPQ4019, IPQ5018, IPQ6018, IPQ8064, IPQ8074, Kamorta, MDM9150, MDM9607, MDM9650, MSM8905, MSM8917, MSM8953, Nicobar, QCA6390, QCA9531, QCM2150, QCS404, QCS405, QCS605, QCS610, QM215, QRB5165, Rennell, SA415M, SA515M, SA6155P, SA8155P, Saipan, SC8180X, SDM429, SDM429W, SDM439, SDM450, SDM632, SDM660, SDM670, SDM710, SDM845, SDX55, SM6150, SM7150, SM8150, SM8250, SXR1130, SXR2130",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2020-11125"
    },
    {
      "type": "WEB",
      "url": "https://www.qualcomm.com/company/product-security/bulletins/october-2020-bulletin"
    },
    {
      "type": "WEB",
      "url": "https://www.qualcomm.com/company/product-security/bulletins/october-2020-security-bulletin"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-787"
    ],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2020-11-02T07:15:00Z"
  }
}