{
  "schema_version": "1.4.0",
  "id": "GHSA-9qhv-29p6-wwp6",
  "modified": "2022-05-24T17:23:53Z",
  "published": "2022-05-24T17:23:53Z",
  "aliases": [
    "CVE-2020-1650"
  ],
  "details": "On Juniper Networks Junos MX Series with service card configured, receipt of a stream of specific packets may crash the MS-PIC component on MS-MIC or MS-MPC. By continuously sending these specific packets, an attacker can repeatedly bring down MS-PIC on MS-MIC/MS-MPC causing a prolonged Denial of Service. This issue affects MX Series devices using MS-PIC, MS-MIC or MS-MPC service cards with any service configured. This issue affects Juniper Networks Junos OS on MX Series: 17.2R2-S7; 17.3R3-S4, 17.3R3-S5; 17.4R2-S4 and the subsequent SRs (17.4R2-S5, 17.4R2-S6, etc.); 17.4R3; 18.1R3-S3, 18.1R3-S4, 18.1R3-S5, 18.1R3-S6, 18.1R3-S7, 18.1R3-S8; 18.2R3, 18.2R3-S1, 18.2R3-S2; 18.3R2 and the SRs based on 18.3R2; 18.4R2 and the SRs based on 18.4R2; 19.1R1 and the SRs based on 19.1R1; 19.2R1 and the SRs based on 19.2R1; 19.3R1 and the SRs based on 19.3R1.",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2020-1650"
    },
    {
      "type": "WEB",
      "url": "https://kb.juniper.net/JSA11037"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-400"
    ],
    "severity": "MODERATE",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2020-07-17T19:15:00Z"
  }
}