{
  "schema_version": "1.4.0",
  "id": "GHSA-g744-hv99-8369",
  "modified": "2022-05-14T03:18:34Z",
  "published": "2022-05-14T03:18:34Z",
  "aliases": [
    "CVE-2018-5515"
  ],
  "details": "On F5 BIG-IP 13.0.0-13.1.0.5, using RADIUS authentication responses from a RADIUS server with IPv6 addresses may cause TMM to crash, leading to a failover event.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.0/AV:N/AC:H/PR:H/UI:N/S:U/C:N/I:N/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2018-5515"
    },
    {
      "type": "WEB",
      "url": "https://support.f5.com/csp/article/K62750376"
    },
    {
      "type": "WEB",
      "url": "http://www.securityfocus.com/bid/104099"
    },
    {
      "type": "WEB",
      "url": "http://www.securitytracker.com/id/1040802"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-20"
    ],
    "severity": "MODERATE",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2018-05-02T13:29:00Z"
  }
}