{
  "schema_version": "1.4.0",
  "id": "GHSA-g7xv-jv8r-q9x7",
  "modified": "2022-05-24T16:51:25Z",
  "published": "2022-05-24T16:51:25Z",
  "aliases": [
    "CVE-2019-2301"
  ],
  "details": "Possibility of out-of-bound read if id received from SPI is not in range of FIFO in Snapdragon Auto, Snapdragon Compute, Snapdragon Consumer IOT, Snapdragon Industrial IOT, Snapdragon Mobile, Snapdragon Wearables, Snapdragon Wired Infrastructure and Networking in IPQ4019, IPQ8064, MSM8909W, MSM8996AU, QCA9980, QCS605, Qualcomm 215, SD 425, SD 439 / SD 429, SD 450, SD 625, SD 632, SD 636, SD 712 / SD 710 / SD 670, SD 820A, SD 845 / SD 850, SD 855, SDM439, SDM660, SDX24",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2019-2301"
    },
    {
      "type": "WEB",
      "url": "https://www.codeaurora.org/security-bulletin/2019/07/01/july-2019-code-aurora-security-bulletin"
    }
  ],
  "database_specific": {
    "cwe_ids": [],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2019-07-25T17:15:00Z"
  }
}