{
  "schema_version": "1.4.0",
  "id": "GHSA-g76q-jc2x-v9j3",
  "modified": "2022-05-01T18:33:38Z",
  "published": "2022-05-01T18:33:37Z",
  "aliases": [
    "CVE-2007-5475"
  ],
  "details": "Multiple buffer overflows in the Marvell wireless driver, as used in Linksys WAP4400N Wi-Fi access point with firmware 1.2.17 on the Marvell 88W8361P-BEM1 chipset, and other products, allow remote 802.11-authenticated users to cause a denial of service (wireless access point crash) and possibly execute arbitrary code via an association request with long (1) rates, (2) extended rates, and unspecified other information elements.",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2007-5475"
    },
    {
      "type": "WEB",
      "url": "http://secunia.com/advisories/37345"
    },
    {
      "type": "WEB",
      "url": "http://www.securityfocus.com/archive/1/507781/100/0/threaded"
    },
    {
      "type": "WEB",
      "url": "http://www.vupen.com/english/advisories/2009/3239"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-119"
    ],
    "severity": "MODERATE",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2009-11-12T23:30:00Z"
  }
}