{
  "schema_version": "1.4.0",
  "id": "GHSA-g833-8mx8-2ffm",
  "modified": "2022-05-01T02:20:32Z",
  "published": "2022-05-01T02:20:32Z",
  "aliases": [
    "CVE-2005-3722"
  ],
  "details": "The SNMP v1/v2c daemon in Hitachi IP5000 VOIP WIFI Phone 1.5.6 allows remote attackers to gain read or write access to system configuration using arbitrary SNMP credentials.",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2005-3722"
    },
    {
      "type": "WEB",
      "url": "http://marc.info/?l=full-disclosure&m=113217425618951&w=2"
    },
    {
      "type": "WEB",
      "url": "http://secunia.com/advisories/17628"
    },
    {
      "type": "WEB",
      "url": "http://www.hitachi-cable.co.jp/ICSFiles/infosystem/security/76659792_e.pdf"
    }
  ],
  "database_specific": {
    "cwe_ids": [],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2005-11-21T11:03:00Z"
  }
}