{
  "schema_version": "1.4.0",
  "id": "GHSA-f4fc-q79g-8f2p",
  "modified": "2022-05-17T05:18:43Z",
  "published": "2022-05-17T05:18:43Z",
  "aliases": [
    "CVE-2012-1800"
  ],
  "details": "Stack-based buffer overflow in the Profinet DCP protocol implementation on the Siemens Scalance S Security Module firewall S602 V2, S612 V2, and S613 V2 with firmware before 2.3.0.3 allows remote attackers to cause a denial of service (device outage) or possibly execute arbitrary code via a crafted DCP frame.",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2012-1800"
    },
    {
      "type": "WEB",
      "url": "http://osvdb.org/81034"
    },
    {
      "type": "WEB",
      "url": "http://support.automation.siemens.com/WW/view/en/59869684"
    },
    {
      "type": "WEB",
      "url": "http://www.siemens.com/corporate-technology/pool/de/forschungsfelder/siemens_security_advisory_ssa-268149.pdf"
    },
    {
      "type": "WEB",
      "url": "http://www.us-cert.gov/control_systems/pdf/ICSA-12-102-05.pdf"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-119"
    ],
    "severity": "MODERATE",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2012-04-18T10:33:00Z"
  }
}